  

                



Figure : Response on EE to leakage current (EE at 0V output)



