

Figure 1: Gas line opened to verify He detection

