(Normal Camera) Camera container filled with Argon.

-Place under Vacuum, monitor w/ RGA.

-Start RGA as soon as Turbo pumps reach speed.

Thursday, November 24, 2016, 11:43 Pump down started. Camera and case placed near RGA









20 mins after start of RGA





Anomaly on Nitrogen noticed around 00:37:00 to 01:25:00

Argon appeared stable.



     