(Normal Camera) Camera container filled with Argon.

-Place under Vacuum, monitor w/ RGA.

-Start RGA as soon as Turbo pumps reach speed.













