**Target Test (Fully Cleaned vs Crystal Clean only).**

For all tests:

-Start Turbo pumps & Ion gauge as soon as available on ISAC TEST STAND VACUUM Screen.

- Ensure previous test turbos are off by 8:15 and started venting by 9:15am to meet timeline.

-Start Roughing by 10:10am +/- 1 minute.

-TGHT / TBHT ramping starts @ 8:30am. 2A per min to 580A / 200A

ALL START TIMES MUST BE CONSISTANT.

**\*\*\*Pre-outgassed\*\*\* Heat Shield W.O# 42738-1**: Includes insulators, new Al grounded 9-pin, bracket, & gripper arms. Blank/Plate. No source cup/EE.

**HP-SIS Target # 42218-8:** Crystal Clean only. (Long test)

Monday, July 24, 2017, 09:46: HS removed from test stand. Exchange target.

Monday, July 24, 2017, 10:08: Target # 42218-8 placed into test stand. Door open for 22 minutes.

Monday, July 24, 2017, 10:10: Roughing.

Monday, July 24, 2017, 10:10: Doors sealed for roughing.

Monday, July 24, 2017, 10:11: BV1B OPEN. Opened @ 306T.

Monday, July 24, 2017, 10:29: Both Turbo pumps started.

























































