

FEBIAD COIL TEST 6

SILVER BOLTS USED ON COIL, TGHT, TBHT.


End Caps installed.





Restart due to shut down.





Oct 11, 2018





























































**ANODE / CATHODE PS REQUIRES REVERSAL!!!!**






























<http://isacwserv.triumf.ca/onlylocal/isactdata/save_restore/masscorr/2018-10-12-13-52%20POS%20Cathode%20-%20200V%20Anode>











<http://isacwserv.triumf.ca/onlylocal/isactdata/save_restore/masscorr/2018-10-12-13-52%20POS%20Cathode%20-%200V%20Anode%20-%2050A%20Coil>

Anode @ 0 V – Coil @ 50 A.

