{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["Target Index","TargetOrder","Vault","miniVault","Summary","VaultPlan","Pails","DaysToShip"],"not_rendered":{"charts":9,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":2,"pivot_tables":7},"unopened":[{"sheet":"DaysToShip","index":7,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Target Index","index":0,"n_rows":202,"n_cols":58,"rows_kept":202,"cut":false,"hidden":false,"merged":[]}
[null,"Show",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Table1[Net Charge \n'[uAh']])","v":2935703.1399999997}]
["ID","Material","No","HP/LP","IS","Note","TS","TM","Year","Month","Day","Schedule","DocuShare","URL","Target Mtl\n[g]","Backing Mtl\n[g]","Weight\n[kg]","Installed","Heaters\n/ ECR On","Online p+","Offline p+","Removed","Impedance \n[mΩ]","Rated p+ \n[uA]","Peak p+ \n[uA]","Net Charge \n[uAh]","Est p+ Charge","BIAS\n[kV]","Target ID","Assay 1 Date","Assay 1\n[uSv/h]@1m","Assay 2 Date","Assay 2\n[uSv/h]@1m","Assay 3 Date","Assay 3\n[uSv/h]@1m","Assay 4 Date","Assay 4\n[uSv/h]@1m","Assay 5 Date","Assay 5\n[uSv/h]@1m","Date of being sent to Mini Storage","Mini Storage location","Date removed from Mini Storage","Shipping Date","Dose rate OC F-308 uSv/h\n[mSv/h]","Dose rate@1m F-308 uSv/h","Days to ship [d]","Calc ship days","Optimistic","Estimated current","Schedule start","Schedule end","Estimated ship days","Estimated ship years","Vault location","Pail","Vault comment","Target Assayed","Name"]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb#10"},"Nb",10,"LP","IGLIS",null,"ITW","TM2",null,null,null,144,"Link",null,null,{"$f":"29.049-22.009","v":7.0399999999999991},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb#10"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-Nb#10-LP-IGLIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#42"},"UC",42,"LP","SIS",null,"ITE","TM4",null,null,null,144,"Link ",null,null,{"$f":"29.049-22.009","v":7.0399999999999991},null,"2023-07-18","2023-07-22","2023-07-25",null,null,13.7,20,null,null,null,null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#42"},"2023-09-01",34900,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"6B",282,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#42-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#45"},"SiC",45,"HP","SIS",null,"ITE","TM4",null,null,null,144,"Link",null,null,{"$f":"29.049-22.009","v":7.0399999999999991},null,"2023-06-13","2023-06-19","2023-06-20","2023-07-11","2023-07-18",12.3,70,70,29342.01,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.5491366319999982E+20},42,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#45"},"2023-07-27",138000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1467.1005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1408.4164799999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"3C",280,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#45-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"TiC#6"},"TiC",6,"HP","FEBIAD",null,"ITW","TM2",null,null,null,144,"Link",null,null,{"$f":"29.049-22.009","v":7.0399999999999991},null,"2023-05-29","2023-06-08","2023-06-09","2023-07-25","2023-08-08",12.8,100,90,22481,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.0177591999999993E+20},46,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"TiC#6"},"2023-08-23",151000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":719.39200000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":719.39200000000005},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"6A",232,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-TiC#6-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"TiC#5"},"TiC",5,"LP","FEBIAD",null,"ITE","TM4",2023,6,21,144,"Link",null,null,{"$f":"29.049-22.009","v":7.0399999999999991},null,"2023-05-09","2023-05-24","2023-05-31","2023-06-13","2023-06-13",16,"55/70",65,7499.37,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.6738593840000002E+20},45,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"TiC#5"},"2023-06-21",40000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":239.97984},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":239.97984},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"3A",279,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-TiC#5-LP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#41"},"UC",41,"LP","SIS",null,"ITE","TM4",2023,1,30,143,"Link",null,null,{"$f":"29.049-22.009","v":7.0399999999999991},null,"2022-11-29","2022-12-05","2022-12-06","2022-12-21","2023-01-24",14.8,20,18,4038.64,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.01424448E+19},40,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#41"},"2023-01-30",14000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":468.48223999999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":306.93663999999995},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"1C",231,"Pail is likely contaminated, Contains two proton beam window without copper cooling lines in addition to the target\n\nThis pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#41-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#40"},"UC",40,"LP","SIS",null,"ITW","TM2",2023,1,11,143,"Link",null,null,7.0399999999999991,null,"2022-11-15","2022-11-16","2022-11-17","2022-12-06","2023-01-09",14.25,20,19,6196.91,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.3831503119999997E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#40"},"2023-01-11",15600,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":718.84156000000007},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":470.96515999999997},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"1B",278,"contains one proton beam window without copper cooling lines in addition to the target\n\nThis pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-UC#40-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"C#4"},"C",4,"LP","SIS",null,"ITE","TM4",2022,11,24,143,"Link",null,null,7.0399999999999991,null,"2022-10-11","2022-10-18","2022-10-20","2022-11-17","2022-11-22",15.52,90,78,28829.7,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.4347890400000003E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"C#4"},"2022-11-24",164000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"4C",277,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-C#4-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#39"},"UC",39,"LP","IGLIS",null,"ITW","TM2",2022,11,3,142,"Link",null,null,7.0399999999999991,null,"2022-09-13","2022-09-17","2022-09-20","2022-10-03","2022-11-01",13.78,20,16,4151.79,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.2667952799999984E+19},42,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#39"},"2022-11-03",14400,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":481.60764},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":315.53604000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"4B",276,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-UC#39-LP-IGLIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#44"},"SiC",44,"HP","FEBIAD",null,"ITE","TM4",2022,10,13,142,"Link",null,null,7.0399999999999991,null,"2022-08-16","2022-08-17","2022-08-31","2022-09-11","2022-10-03",10.27,70,60,11419.5,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.5488323999999997E+20},36.6,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#44"},"2022-10-13",42600,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":570.97500000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":548.13599999999997},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"4A",275,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#44-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#38"},"UC",38,"LP","SIS",null,"ITW","TM2",2022,9,15,142,"Link",null,null,7.0399999999999991,null,"2022-07-26","2022-07-28","2022-08-02","2022-08-30","2022-09-06",13.54,20,20,8011.88,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.7882516159999997E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#38"},"2022-09-15",33300,"2022-12-16",{"$f":"4.78*1000","v":4780},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":929.37808000000007},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":608.90287999999998},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"1A",274,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-UC#38-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#64"},"Ta",64,"LP","SIS",null,"ITE","TM4",2022,8,18,142,"Link",null,null,7.0399999999999991,null,"2022-06-28","2022-07-04","2022-07-04","2022-08-02","2022-08-09",13.13,"40/60",60,15070.79,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.3638003279999998E+20},22.468,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#64"},"2022-08-18",86600,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":512.40686000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":421.98212000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"5C",273,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#64-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#43"},"SiC",43,"HP","FEBIAD",null,"ITW","TM2",2022,7,28,142,"Link",null,null,7.0399999999999991,null,"2022-0620","2022-06-21","2022-06-22","20022-07-02","2022-07-19",12.72,75,65,10192.27,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.2749146639999998E+20},36.700000000000003,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#43"},"28/07/2022",47800,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":509.61350000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":489.22896000000003},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"5A",272,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-SiC#43-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#42"},"SiC",42,"HP","FEBIAD",null,"ITW","TM2",2022,7,6,142,"Link",null,null,7.0399999999999991,null,"2022-06-07","2022-06-10","2022-06-14","2022-06-17","2022-06-20",12.26,70,80,1307.21,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.9176927199999996E+19},42,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#42"},"2022-07-06",9140,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":65.360500000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":62.746080000000006},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"2B",271,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-SiC#42-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#37"},"UC",37,"P2N","SIS",null,"ITE","TM4",2022,6,23,142,"Link",null,null,7.0399999999999991,null,"2022-05-18","2022-05-26","2022-06-01","2022-06-14","2022-06-21",5.21,16000,80,7400.87,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.6518741839999998E+20},42,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#37"},"23/06/2022",63200,"2022-12-16",{"$f":"3.86*1000","v":3860},null,null,null,null,null,null,"2023-01-06","M3","2023-01-17",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":858.50092000000006},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":562.46611999999993},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,228,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#37-P2N-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#63"},"Ta",63,"LP","SIS",null,"ITE","TM4",2022,1,20,141,"Link",null,null,7.0399999999999991,null,"2021-11-30","2021-12-03","2021-12-07","2021-12-21","2022-01-18",14.7,"40/60",50,13891.88,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.100667616E+20},22.529,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#63"},"20/01/2022",410000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":472.32391999999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":388.97264000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"3B",266,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#63-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#36"},"UC",36,"LP","SIS",null,"ITW","TM2",2022,1,12,141,"Link",null,null,7.0399999999999991,null,"2021-11-09","2021-11-14","2021-11-17","2021-12-07","2022-01-10",14.8,20,19,5770.26,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.287922032E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#36"},"2022-01-12",19600,"2022-01-28",10700,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":669.35016000000007},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":438.53976},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"2A",265,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-UC#36-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#35"},"UC",35,"LP","IG-LIS",null,"ITE","TM4",2021,11,26,141,"Link",null,null,null,null,"2021-10-07","2021-10-18","2021-10-26","2021-11-16","2021-11-23",13.1,"20/40",19,4710.3500000000004,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.05135012E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#35"},"2021-11-26",25700,"2022-01-31",5870,"2022-12-16",748,null,null,null,null,"2022-12-16",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":546.40060000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":357.98660000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,264,null,"Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#35-LP-IG-LIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"C#3"},"C",3,"LP","SIS",null,"ITW","TM2",2021,11,5,141,"Link",null,null,{"$f":"29.049-22.009","v":7.0399999999999991},null,"2021-09-27","2021-10-10","2021-10-13","2021-10-26","2021-11-09",15.55,90,75,15197.92,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.392175744E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"C#3"},"2021-11-10",37900,"2022-01-28",10800,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"2C",270,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-C#3-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#40"},"SiC",40,"HP","SIS",null,"ITE","TM4",2021,9,14,140,"Link",null,null,null,null,"2021-09-07","2021-09-10","N/A","N/A","2021-09-14",null,75,0,0,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":0},38,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#40"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":0},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":0},60,"2021-09-14","2021-09-26",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":1313.28},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":3.5980273972602741},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#40-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#34"},"UC",34,"LP","SIS",null,"ITW","TM2",2021,8,25,140,"Link",null,null,null,null,"2021-08-10","2021-08-22","2021-08-25","2021-09-11","2021-09-21",14.6,null,18,5750.14,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.283431248E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#34"},"2021-09-22",419000,"2022-01-27",4730," 2022-12-16",809,null,null,null,null," 2022-12-16",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":667.01624000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":437.01064000000002},20,"2021-08-25","2021-09-14",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":729.6},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.9989041095890412},null,268,"Pail changed from 258 to 268","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-UC#34-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#62"},"Ta",62,"LP","SIS",null,"ITE","TM4",2021,7,28,140,"Link",null,null,null,null,"2021-07-20","2021-07-26","2021-07-29","2021-08-24","2021-08-31",13.95,"50/70",70,15969.23,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.5643321359999992E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#62"},"2021-09-17",58000,"2022-01-27",16900," 2022-12-16",{"$f":"3.6*1000","v":3600},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":542.95382000000006},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":447.13844},40,"2021-07-28","2021-08-25",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":752.64},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.0620273972602741},"7A",256,"2022-12-16 moved from 7A to 7B in vault. - AN Pail placed back in 7A. -TC\nDisc in bottom of pail was not installed pail will need repacking. This pail is likely contaminated and also contains 2A2M19.\n\nThis pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#62-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#33"},"UC",33,"LP","SIS",null,"ITW","TM2",2021,6,29,140,"Link",null,null,null,null,"2021-06-22","2021-06-24","2021-06-30","2021-07-27","2021-08-03",13.95,"20/40",22,6599.58,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.4730262559999997E+20},40,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#33"},"2021-08-06",39900,"2022-01-27",4070,"2022-12-16",708,null,null,null,null,"2022-12-16",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":765.55128000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":501.56808000000001},20,"2021-06-29","2021-07-28",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":1057.92},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.8984109589041096},null,267,"First one done from the NHC pail changed from 255 to 267","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-UC#33-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#32"},"UC",32,"P2N","SIS",null,"ITE","TM4",2021,6,16,140,"Link",null,null,null,null,"2021-06-01","2021-06-10","2021-06-15","2021-06-24","2021-07-06",4.92,98,50,2934.66,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.55016112E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#32"},"2021-07-09",21200,"2022-01-27",2760,null,null,null,null,null,null,"2022-05-19",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":340.42056000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":223.03415999999999},20,"2021-06-16","2021-06-29",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":474.24},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.2992876712328767},null,233,"Changed from pail 254 to 233","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#32-P2N-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb#9"},"Nb",9,"LP","SS",null,"ITW","TM2",2020,12,1,139,"Link",null,null,null,null,"2020-11-24","2020-11-26","2020-12-01","2020-12-21","2021-01-19",13.3,55,50,18619,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.1557608E+20},50,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb#9"},"2021-01-21",149000,"2022-01-31",9080,"2022-12-16",{"$f":"1.98*1000","v":1980},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":567.87950000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":428.23699999999997},40,"2020-12-01","2020-12-22",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":463.68},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.2703561643835617},"6C",246,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-Nb#9-LP-SS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#61"},"Ta",61,"LP","SIS",null,"ITE","TM4",2020,11,10,139,"Link",null,null,null,null,"2020-11-05","2020-11-09","2020-11-11","2020-12-01","2021-01-08",13.4,"40/60",35,11870,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.649384E+20},48,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#61"},"2021-01-13",41600,"2022-01-31",3620,"2022-12-16",{"$f":"1.56*1000","v":1560},null,null,null,null,"2022-12-16",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":403.58000000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":332.36},40,"2020-11-10","2020-12-01",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":564.48},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.5465205479452055},null,245,null,"Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#61-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"C#2"},"C",2,"LP","SIS",null,"ITW","TM2",2020,10,22,139,"Link",null,null,null,null,"2020-10-20","2020-10-22","2020-10-26","2020-11-10","2020-11-17",15.8,"95/100",90,18131,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.0468392E+20},40,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"C#2"},"2020-11-19",185000,"2022-01-28",3230,null,null,null,null,null,null,"2022-05-19",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},100,"2020-10-22","2020-11-10",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,235,null,"Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-C#2-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#31"},"UC",31,"P2N","SIS",null,"ITE","TM4",2020,10,6,138,"Link",null,null,null,null,"2020-09-23","2020-10-01","2020-10-19","2020-10-25","2020-11-03",21.8,98,90,1686,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.763152E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#31"},"2020-11-12",3710,null,null,null,null,null,null,null,null,"2021-05-14",null,"2021-05-19",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":195.57600000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":128.136},20,"2020-09-15","2020-09-28",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":474.24},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.2992876712328767},null,224,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#31-P2N-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#60"},"Ta",60,"LP","SIS",null,"ITW","TM2",2020,9,17,138,"Link",null,null,null,null,"2020-08-26","2020-09-14","2020-09-17","2020-10-06","2020-10-16",14.3,40,40,11161,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.4911352E+20},50,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#60"},"2020-10-21",83200,"2022-01-27",3700," 2022-12-16",{"$f":"1.38*1000","v":1380},null,null,null,null," 2022-12-16",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":379.47400000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":312.50799999999998},40,"2020-09-17","2020-10-06",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":510.72},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.3992328767123288},null,239,null,"Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-Ta#60-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#30"},"UC",30,"LP","SIS",null,"ITE","TM4",2020,8,25,138,"Link",null,null,null,null,"2020-07-03","2020-08-24","2020-08-25","2020-09-17","2020-09-22",12.8,"20/40",25,7079,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.5800328E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#30"},"2020-09-24",81500,"2022-01-27",1240,null,null,null,null,null,null,"2022-05-19",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":821.16399999999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":538.00400000000002},20,"2020-07-28","2020-08-18",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":766.07999999999993},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.098849315068493},null,238,null,"Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#30-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"C#1"},"C",1,"LP","SIS",null,"ITW","TM2",2020,7,15,138,"Link",null,null,null,null,"2020-06-17","2020-08-14","2020-08-15","2020-08-16","2020-08-18",15.5,100,1,0,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":0},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"C#1"},"2020-08-27",200,null,null,null,null,null,null,null,null,"2021-03-25",null,"2021-03-26","2021-03-26",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":222},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},100,"2020-07-15","2020-07-28",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,237,"Contains broken 2A2M19. Moved to cyclotron vault 2021-03-26.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-C#1-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#39"},"SiC",39,"HP","FEBIAD",null,"ITE","TM2",2019,12,3,137,"Link",null,null,null,null,"2019-11-29","2019-11-30","2019-12-02","2019-12-14","2020-02-27",11.9,"75/100",55,13743.37,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.0675201840000002E+20},40,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#39"},"2020-03-06",30600,"2022-01-31",3160,null,null,null,null,null,null,"2022-05-19",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":687.16850000000011},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":659.68176000000005},15,"2019-12-03","2019-12-22",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":519.84},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.4242191780821918},null,227,"Contamination might be on lid","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM2-SiC#39-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#38"},"SiC",38,"HP","FEBIAD",null,"ITE","TM2",2019,11,20,137,"Link",null,null,null,null,"2019-11-12","2019-11-14","2019-11-20","2019-11-26","2019-11-26",12.1,"70/100",60,1541.79,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.44127528E+19},16.3,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#38"},"2019-12-03",22200,"2021-11-18",290,null,null,null,null,null,null,"2021-11-18",null,"2021-11-29",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":77.089500000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":74.005920000000003},60,"2019-11-20","2019-12-03",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":1422.72},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":3.8978630136986303},null,205,"Check for contamination on lid",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM2-SiC#38-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#29"},"UC",29,"LP","SIS",null,"ITW","TM4",2019,10,30,137,"Link",null,null,null,null,"2019-10-24","2019-10-29","2019-10-30","2019-12-21","2020-02-04",13.85,"20/40",20,11913,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.6589816E+20},35,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#29"},"2020-02-07",22400,"2021-11-18",922,null,null,null,null,null,null,"2021-11-18",null,"2021-11-29",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1381.9080000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":905.38800000000003},15,"2019-10-30","2019-11-20",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":574.55999999999995},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.5741369863013697},null,225,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM4-UC#29-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#59"},"Ta",59,"LP","SIS",null,"ITE","TM2",2019,10,15,137,"Link",null,null,null,null,"2019-10-07","2019-10-11","2019-10-15","2019-10-29","2019-11-05",12.7,"40/60",40,8117.5,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.811826E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#59"},"2019-11-08",121000,"2022-01-31",1680,null,null,null,null,null,null,"2022-05-19",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":275.995},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":227.29},60,"2019-10-15","2019-10-29",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":564.48},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.5465205479452055},null,220,null,"Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM2-Ta#59-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#28"},"UC",28,"LP","SIS",null,"ITW","TM4",2019,9,17,136,"Link",null,null,null,null,"2019-10-04","2019-10-07","2019-10-09","2019-10-15","2019-10-22",12.3,"20/40",15,1792.36,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.0005475199999992E+19},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#28"},"2019-10-28",12600,"2019-12-05",3370,null,null,null,null,null,null,"2020-02-20",null,"2020-02-21","2020-06-17",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":246},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":207.91376},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":136.21935999999999},20,"2019-09-17","2019-10-15",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":1021.4399999999999},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.7984657534246575},null,219,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM4-UC#28-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"ZrC#8"},"ZrC",8,"LP","SIS",null,"ITE","TM2",2019,8,27,136,"Link",null,null,null,null,"2019-08-15","2019-08-17","2019-08-20","2019-09-17","2019-09-30",19.440000000000001,"55/70",70,28196.73,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.2935101359999982E+20},25,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"ZrC#8"},"2019-10-02",205000,"2019-12-10",74800,"2022-01-31",3050,"2022-12-16",{"$f":"1.05*1000","v":1050},null,null,"2023-01-06","M2","2023-01-17",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1409.8365000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1015.0822799999999},50,"2019-08-27","2019-09-17",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":907.19999999999993},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.4854794520547943},null,217,"This pail also contains, wire, a wirescanner, IGM guage, target bolts and water block bolts","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM2-ZrC#8-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#27"},"UC",27,"LP","SIS",null,"ITW","TM4",2019,8,7,136,"Link",null,null,null,null,"2019-09-10","2019-09-15","2019-09-19","2019-09-30","2019-10-03",13.48,"16/40",20,2539.23,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.66756136E+19},25,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#27"},"2019-10-09",22900,"2019-12-05",4230,null,null,null,null,null,null,"2021-05-20",null,"2021-05-21",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":294.55068},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":192.98148},20,"2019-08-07","2019-08-27",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":729.6},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.9989041095890412},null,218,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM4-UC#27-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#58"},"Ta",58,"LP","SIS",null,"ITE","TM2",2019,6,19,136,"Link",null,null,null,null,"2019-05-17","2019-06-04","2019-06-17","2019-08-11","2019-08-13",15.4,"40/60",50,50808.75,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.1340513E+21},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#58"},"2019-08-19",311000,"2019-12-10",52500,"2022-01-31",7120,"2022-12-16",{"$f":"4.21*1000","v":4210},null,null,"2023-01-06","M1","2023-01-17",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1727.4975000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1422.645},50,"2019-06-19","2019-08-07",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":1646.4},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":4.5106849315068498},null,211,null,"Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM2-Ta#58-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#26"},"UC",26,"LP","IG-LIS",null,"ITE","TM4",2018,11,27,135,"Link",null,null,null,null,"2018-12-04","2018-12-07","2018-12-12","2018-12-21","2019-04-30",12.58,40,20,2154.89,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.8097144799999992E+19},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#26"},"2019-05-02",2420,"2019-12-05",620,null,null,null,null,null,null,"2020-02-19",null,"2020-02-21","2020-06-17",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":544},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":249.96724},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":163.77163999999999},10,"2018-11-27","2018-12-22",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":456},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.2493150684931507},null,209,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#26-LP-IG-LIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#25"},"UC",25,"LP","SIS",null,"ITW","TM2",2018,11,7,135,"Link",null,null,null,null,"2018-11-06","2018-11-08","2018-11-21","2018-12-11","2019-01-09",13.3,10,9.8000000000000007,3863.44,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.62319808E+19},25.9,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#25"},"2019-01-11",12800,"2019-11-04",1560,"2019-12-11",1330,"2020-10-30",529,null,null,"2020-10-30",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":448.15904},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":293.62144000000001},10,"2018-11-07","2018-11-27",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":364.8},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":0.99945205479452059},null,244,"This pail is one with the thicker steel. Pail changed from 204 to 244","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-UC#25-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#57"},"Ta",57,"LP","SIS",null,"ITE","TM4",2018,10,2,135,"Link",null,null,null,null,"2018-10-09","2018-10-13","2018-10-16","2018-11-21","2018-11-27",14.2,"40/60",55,21457.02,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.7892068639999997E+20},25,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#57"},"2018-11-30",139000,"2019-11-04",8150,"2021-11-17",3270,null,null,null,null,"2021-11-17",null,"2021-11-29",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":729.53868000000011},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":600.79656},40,"2018-10-02","2018-11-07",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":967.68000000000006},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.6511780821917812},null,174,"Pail switched from 172 to 263","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#57-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"nSiC#1"},"nSiC",1,"LP","SIS","nano","ITW","TM2",2018,9,25,134,"Link",null,null,null,null,"2018-09-20","2018-09-24","2018-09-25","2018-10-16","2018-10-30",14.3,50,50,3782.78,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.44316496E+19},25,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"nSiC#1"},"2018-11-02",13600,"2019-12-09",796,"2020-02-19",457,null,null,null,null,"2020-02-19",null,"2020-02-21","2020-06-17",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":610},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":189.13900000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":181.57344000000001},30,"2018-09-25","2018-10-09",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":483.84000000000003},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.3255890410958906},null,172,"Pail switched from 172 to 226","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-nSiC#1-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#24"},"UC",24,"LP","SIS",null,"ITE","TM4",2018,9,12,134,"Link",null,null,null,null,"2018-09-04","2018-09-07","2018-09-11","2018-09-25","2018-10-02",12.8,10,9.8000000000000007,2440,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.44608E+19},22.5,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#24"},"2018-10-05",22100,"2019-11-01",838,null,null,null,null,null,null,"2019-11-14",null,"2020-01-13","2020-06-17",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":631},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":283.04000000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":185.44},10,"2018-09-11","2018-09-25",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":255.35999999999999},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":0.69961643835616438},null,221,"Pail switched from 171 to 221","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#24-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#23"},"UC",23,"LP","FEBIAD","CTL","ITW","TM2",2018,8,22,134,"Link",null,null,null,null,"2018-08-14","2018-08-16","2018-08-23","2018-09-11","2018-09-18",11.8,10,9.8000000000000007,3999.46,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.92679472E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#23"},"2018-09-25",26700,"2019-11-01",1070,null,null,null,null,null,null,"2019-11-14",null,"2020-01-13","2020-06-17",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":645},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":463.93736000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":303.95895999999999},10,"2018-08-21","2018-09-11",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":383.03999999999996},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.0494246575342465},null,222,"Pail switched from 170 to 222","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-UC#23-LP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#56"},"Ta",56,"HP","SIS",null,"ITE","TM4",2018,8,1,134,"Link",null,null,null,null,"2018-07-23","2018-07-25","2018-07-27","2018-08-21","2018-08-28",10.9,100,60,23481,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.2409592E+20},22.5,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#56"},"2018-08-30",251000,"2019-11-04",9130,"2021-10-29",3860,null,null,null,null,"2021-10-29",null,"2021-11-29",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":798.35400000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":657.46799999999996},60,"2018-08-01","2018-08-21",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":806.4},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.2093150684931504},null,269,"Pail switched from 169 to 269","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#56-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb#8"},"Nb",8,"HP","SIS",null,"ITW","TM2",2018,7,11,134,"Link",null,null,null,null,"2018-07-03","2018-07-05","2018-07-11","2018-07-22","2018-07-31",12.9,100,65,5305.78,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.1842500959999998E+20},12.5,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb#8"},"2018-08-02",71100,"2019-11-04",2740,null,null,null,null,null,null,"2021-05-14",null,"2021-05-19",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":161.82629},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":122.03294},90,"2018-07-11","2018-08-01",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":1043.28},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.8583013698630135},null,247,"Pail switched from 168 to 247","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-Nb#8-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#22"},"UC",22,"LP","SIS",null,"ITE","TM4",2018,6,14,134,"Link",null,null,null,null,"2018-06-06","2018-06-12","2018-06-14","2018-07-10","2018-07-17",15.7,10,9.8000000000000007,4375.1099999999997,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.76524552E+19},40,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#22"},"2018-07-30",18800,"2019-11-01",850,null,null,null,null,null,null,"2019-11-14",null,"2020-01-13","2020-06-17",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":708},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":507.51276000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":332.50835999999998},10,"2018-06-14","2018-07-11",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":492.47999999999996},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.3492602739726027},null,223,"Pail switched from 167 to 223","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#22-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#55"},"Ta",55,"LP","SIS",null,"ITW","TM2",2017,11,21,133,"Link",null,null,null,null,"2017-11-14","2017-11-16","2017-11-21","2017-12-21","2018-04-09",14.9,45,45,36492.17,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.1450523439999995E+20},25,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#55"},"2018-04-16",30400,"2019-12-09",4000,null,null,null,null,null,null,"2021-05-20",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1240.73378},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1021.78076},40,"2017-11-21","2017-12-13",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":591.36},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.6201643835616439},null,251,"Pail switched from 161 to 251","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-Ta#55-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#37"},"SiC",37,"HP","FEBIAD",null,"ITE","TM4",2017,10,31,133,"Link",null,null,null,null,"2017-10-24","2017-10-27","2017-10-31","2017-11-21","2018-05-01",12.2,75,"40?",23105.08,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.1570538560000007E+20},40,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#37"},"2018-05-05",25800,"2019-12-10",3910,null,null,null,null,null,null,"2021-05-14",null,"2021-05-19",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1155.2540000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1109.04384},60,"2017-10-31","2017-11-21",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":2298.2399999999998},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":6.2965479452054787},null,249,"Pail switched from 165 to 249","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#37-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#54"},"Ta",54,"HP","SIS",null,"ITW","TM2",2017,10,11,133,"Link",null,null,null,null,"2017-10-03","2017-10-08","2017-10-11","2017-10-31","2017-11-07",13,60,50,16731.52,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.7344752639999993E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#54"},"2017-11-13",119000,"2018-03-23",20500,"2019-12-10",3900,"2020-10-30",2380,null,null,"2020-10-30",null,"2020-12-01",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":568.87168000000008},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":468.48256000000003},70,"2017-10-11","2017-10-31",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":940.80000000000007},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.5775342465753428},null,241,"Pail Changed from 157 to 241","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-Ta#54-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#21"},"UC",21,"LP","SIS",null,"ITE","TM4",2017,9,12,132,"Link",null,null,null,null,"2017-09-05","2017-09-07","2017-09-12","2017-10-02","2017-10-17",13.2,9.8000000000000007,9.8000000000000007,3844.1,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.5800312E+19},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#21"},"2017-10-23",27400,"2018-03-23",4050,null,null,null,null,null,null,"2019-04-29",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":445.91560000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":292.15159999999997},10,"2017-09-12","2017-10-01",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":346.56},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":0.94947945205479456},null,216,"Pail changed from 159 to 216","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#21-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#53"},"Ta",53,"HP","SIS",null,"ITW","TM2",2017,8,15,132,"Link",null,null,null,null,"2017-08-08","2017-08-10","2017-08-14","2017-09-11","2017-10-03",12.4,60,60,34980.6,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.8076699199999993E+20},18.5,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#53"},"2017-09-28",244000,"2018-03-23",32700,"2019-12-10",7240,"2021-11-15",1880,null,null,"2021-11-15",null,"2021-11-29",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1189.3404},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":979.45679999999993},70,"2017-08-15","2017-09-12",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":1317.1200000000001},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":3.6085479452054798},null,164,"Pail changed from 164 to 262","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-Ta#53-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#52"},"Ta",52,"LP","SIS",null,"ITE","TM4",2017,7,19,132,"Link",null,null,null,null,"2017-07-11","2017-07-13","2017-07-19","2017-08-05","2017-08-28",12.8,40,40,12933.42,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.886739344E+20},25,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#52"},"2017-08-30",38100,"2018-03-23",6420,"2019-11-04",2260,"2019-12-10",2190,null,null,"2020-01-13",null,"2020-02-21","2020-06-17",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1047},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":439.73628000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":362.13576},40,"2017-07-19","2017-08-15",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":725.76},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.9883835616438357},null,230,"Pail changed from 152 to 230","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#52-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#36"},"SiC",36,"HP","FEBIAD","CTL","ITW","TM2",2017,6,20,132,"Link",null,null,null,null,"2017-06-13","2017-06-16","2017-06-20","2017-07-18","2017-08-01",14.8,70,70,36533.18,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.1542057759999984E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#36"},"2017-08-03",190000,"2017-03-23",21000,"2019-12-11",6000,null,null,null,null,"2021-05-14",null,"2021-05-19",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1826.6590000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1753.5926400000001},60,"2017-06-20","2017-07-19",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":3173.7599999999998},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":8.6952328767123284},null,250,"Pail changed from 151 to 250","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-SiC#36-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#20"},"UC",20,"LP","IG-LIS",null,"ITE","TM4",2017,6,2,132,"Link",null,null,null,null,"2017-05-23","2017-05-26","2017-06-03","2017-06-20","2017-06-26",12.4,10,9.8000000000000007,3330.48,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.43363136E+19},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#20"},"2017-06-29",30100,"2018-03-23",1300,"2019-09-23",390,null,null,null,null,"2019-04-29",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":386.33568000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":253.11648},10,"2017-06-02","2017-06-20",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":328.32},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":0.89950684931506852},null,215,"Pail changed from 150 to 215","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#20-LP-IG-LIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#51"},"Ta",51,"LP","SIS",null,"ITW","TM2",2017,5,5,132,"Link",null,null,null,null,"2017-04-15","2017-04-30","2017-05-05","2017-05-30","2017-06-06",13.5,40,40,19814.8,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.42266336E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#51"},"2017-06-12",144000,"2018-03-23",7730,"2019-11-04",3620,"2019-12-09",3730,"2020-10-30",2040,"2020-10-30",null,"2020-12-01",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":673.70320000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":554.81439999999998},40,"2017-05-05","2017-06-02",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":752.64},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.0620273972602741},null,149,"Pail changed from 149 to 242","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-Ta#51-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#19"},"UC",19,"LP","SIS",null,"ITE","TM4",2017,4,14,132,"Link",null,null,null,null,"2017-04-04","2017-04-06","2017-04-12","2017-05-05","2017-05-16",12.5,10,9.8000000000000007,4401.84,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.82490688E+19},40,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#19"},"2017-05-18",22800,"2018-03-23",1410,"2019-09-23",490,null,null,null,null,"2019-04-29",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":510.61344000000003},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":334.53984000000003},10,"2017-04-14","2017-05-05",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":383.03999999999996},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.0494246575342465},null,214,"Pail changed from 145 to 214","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#19-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#18"},"UC",18,"LP","SIS",null,"ITW","TM2",2016,12,5,131,"Link",null,null,null,null,"2016-11-29","2016-12-02","2016-12-05","2016-12-22","2017-01-24",13.9,10,9.8000000000000007,3289.23,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.34156136E+19},40,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#18"},"2017-01-26",2700,"2017-03-20",3140,null,null,null,null,null,null,"2017-05-02",null,null,"2017-07-07",890,50,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":197},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":381.55068},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":249.98148},10,"2016-12-05","2016-12-20",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":273.59999999999997},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":0.74958904109589031},null,147,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-UC#18-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#50"},"Ta",50,"LP","SIS",null,"ITE","TM4",2016,11,16,131,"Link",null,null,null,null,"2016-11-08","2016-11-11","2016-11-16","2016-12-05","2017-01-25",12.1,40,40,17966.12,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.0100379839999993E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#50"},"2017-01-26",38200,"2017-03-20",16300,"2018-03-23",4020,null,null,null,null,"2018-09-06",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":610.84807999999998},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":503.05135999999999},40,"2016-11-16","2016-12-05",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":510.72},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.3992328767123288},null,148,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#50-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#35"},"SiC",35,"HP","FEBIAD",null,"ITW","TM2",2016,10,25,131,"Link",null,null,null,null,"2016-10-25","2016-10-27","2016-11-02","2016-11-15","2016-11-22",12.2,65,65,16453.12,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.672336384E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#35"},"2016-11-24",228000,"2017-03-20",18500,"2018-03-23",4410,"2019-12-05",2850,null,null,"2020-10-30",null,"2020-12-01",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":822.65599999999995},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":789.74975999999992},60,"2016-10-25","2016-11-16",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":2407.6799999999998},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":6.5963835616438349},null,240,"Pail Changed from 144 to 240","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-SiC#35-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#34"},"SiC",34,"LP","IG-LIS",null,"ITE","TM4",2016,10,4,131,"Link",null,null,null,null,"2016-09-27","2016-10-02","2016-10-05","2016-10-28","2016-11-01",13.6,65,65,14842.55,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.3128571599999992E+20},42,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#34"},"2016-11-03",125000,"2017-03-20",8170,"2018-03-23",3000,null,null,null,null,"2018-09-06",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":742.12750000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":712.44240000000002},40,"2016-10-04","2016-10-25",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":1532.1599999999999},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":4.1976986301369861},null,143,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#34-LP-IG-LIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#49"},"Ta",49,"HP","SIS",null,"ITW","TM2",2016,9,6,131,"Link",null,null,null,null,"2016-08-30","2016-09-02","2016-09-06","2016-09-26","2016-10-11",12.2,60,60,19842.14,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.4287656479999997E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#49"},"2016-10-20",134000,"2017-03-20",19300,"2018-03-23",4650,"2019-11-04",3030,"2019-12-11",2660,"2020-01-13",null,"2020-02-21","2020-06-17",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1360},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":674.63276000000008},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":555.57992000000002},70,"2016-09-06","2016-09-25",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":893.76},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":2.4486575342465753},null,229,"Pail changed from 146 to 229","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-Ta#49-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#17"},"UC",17,"LP","SIS",null,"ITE","TM4",2016,8,15,130,"Link",null,null,null,null,"2016-08-09","2016-08-11","2016-08-15","2016-09-06","2016-09-20",12.6,10,9.8000000000000007,3990.08,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.9058585599999984E+19},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#17"},"2016-09-26",15800,"2017-03-20",1970,null,null,null,null,null,null,"2017-05-02",null,null,"2017-07-07",650,40,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":304},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":462.84928000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":303.24608000000001},10,"2016-08-15","2016-09-06",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":401.28},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.0993972602739726},null,142,"Bolts maybe contmainated","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#17-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#33"},"SiC",33,"HP","SIS",null,"ITW","TM2",2016,7,18,130,"Link",null,null,null,null,"2016-07-12","2016-07-15","2016-07-18","2016-08-15","2016-08-23",12.2,70,70,41366.11,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.2329157519999998E+20},42.9,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#33"},"2016-08-25",295000,"2017-03-20",25100,"2018-03-23",7500,"2019-11-04",4540,"2019-12-09",3390,"2021-05-14",null,"2021-05-19",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":2068.3054999999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1985.5732800000001},60,"2016-07-18","2016-08-15",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":3064.3199999999997},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":8.3953972602739722},null,248,"Pail changed from 141 to 248","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-SiC#33-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#16"},"UC",16,"LP","IG-LIS",null,"ITE","TM4",2016,6,27,130,"Link",null,null,null,null,"2016-06-14","2016-06-24","2016-06-27","2016-07-18","2016-08-02",12.5,10,9.8000000000000007,4078.63,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.1035021599999984E+19},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#16"},"2016-08-30",14100,"2017-03-20",1580,null,null,null,null,null,null,"2017-05-02",null,null,"2017-07-07",610,25,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":354},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":473.12108000000006},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":309.97588000000002},10,"2016-06-27","2016-07-18",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":383.03999999999996},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.0494246575342465},null,140,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#16-LP-IG-LIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#48"},"Ta",48,"HP","SIS",null,"ITW","TM2",2016,5,30,130,"Link",null,null,null,null,"2016-05-25","2016-05-27","2016-05-30","2016-06-27","2016-07-05",11.7,60,60,27344.95,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.1033928400000005E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#48"},"2016-07-11",201000,"2017-03-20",7310,"2018-03-23",5570,"2019-11-04",3630,"2019-12-12",3610,"2020-10-30",null,"2020-12-01",null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":929.7283000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":765.65860000000009},70,"2016-05-30","2016-06-27",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":1317.1200000000001},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":3.6085479452054798},null,139,"Pail changed from 139 to 243","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-Ta#48-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#47"},"Ta",47,"LP","SIS",null,"ITE","TM4",2016,5,6,130,"Link",null,null,null,null,"2016-04-12","2016-05-03","2016-05-06","2016-05-30","2016-06-07",12,40,60,15000.58,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.3481294559999997E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#47"},"2016-06-15",114000,"2016-06-30",42500,"2017-03-20",5920,"2018-03-23",2920,null,null,"2018-09-06",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":510.01972000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":420.01623999999998},40,"2016-05-06","2016-05-30",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":645.12},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":1.7674520547945205},null,137,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#47-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#15"},"UC",15,"LP","SIS",null,"ITW","TM1",2016,4,19,130,"Link",null,null,null,null,"2016-04-05","2016-04-12","2016-04-19","2016-05-06","2016-05-18",13.8,10,9.8000000000000007,2948.56,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.58118592E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#15"},"2016-05-24",14100,"2016-06-30",5270,"2017-03-20",873,null,null,null,null,"2017-05-02",null,null,"2017-07-07",315,15,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":427},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":342.03296},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":224.09055999999998},10,"2016-04-19","2016-05-06",{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":310.08},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":0.84953424657534238},null,136,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-UC#15-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#14"},"UC",14,"LP","SIS",null,"ITE","TM4",2015,12,7,129,"Link",null,null,null,null,"2015-12-01","2015-12-04","2015-12-07","2015-12-22","2016-04-07",13.6,10,9.8000000000000007,2758.24,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.1563916799999992E+19},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#14"},"2016-06-28",1990,null,null,null,null,null,null,null,null,"2016-10-18",null,null,"2017-01-27",420,15,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":402},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":319.95583999999997},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":209.62623999999997},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,135,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#14-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#32"},"SiC",32,"HP","FEBIAD",null,"ITW","TM2",2015,11,10,129,"Link",null,null,null,null,"2015-10-20","2015-10-26","2015-11-14","2015-12-07","2016-03-16",12.2,75,60,28554.5,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.3733644000000003E+20},38.799999999999997,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#32"},"2016-03-22",79700,"2016-06-30",24500,"2017-03-20",8210,"2018-03-23",4160,"2019-09-23",2980,"2019-04-29",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1427.7250000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1370.616},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,213,"Pail changed from 132 to 213","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-SiC#32-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#46"},"Ta",46,"HP","SIS",null,"ITE","TM4",2015,10,6,129,"Link",null,null,null,null,"2015-09-29","2015-10-03","2015-10-06","2015-11-09","2015-11-24",12.1,60,60,17662.509999999998,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.9422722319999992E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#46"},"2015-11-25",265000,"2016-06-30",22000,"2017-03-20",7310,"2018-03-23",3340,null,null,"2018-09-06",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":600.52534000000003},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":494.55027999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,126,"Contains target bits from HC clean up","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#46-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"ZrC#7"},"ZrC",7,"LP","SIS",null,"ITW","TM2",2015,9,8,129,"Link",null,null,null,null,"2015-09-01","2015-09-04","2015-09-08","2015-10-06","2015-10-14",31.2,50,50,16397.099999999999,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.6598327199999997E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"ZrC#7"},"2015-10-23",157000,"2016-06-30",15200,"2017-03-20",3850,null,null,null,null,"2017-10-26",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":819.85500000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":590.29559999999992},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,129,"Contains TM#4 water line","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-ZrC#7-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#13"},"UC",13,"LP","IG-LIS",null,"ITE","TM4",2015,8,7,128,"Link",null,null,null,null,"2015-07-29","2015-08-05","2015-08-08","2015-09-07","2015-09-22",17.2,10,9.8000000000000007,3351.57,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.48070424E+19},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#13"},"2015-09-24",21500,"2016-06-20",1260,null,null,null,null,null,null,"2016-06-30",null,null,"2017-01-27",220,12,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":508},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":388.78212000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":254.71932000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,128,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#13-LP-IG-LIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#31"},"SiC",31,"HP","SIS",null,"ITE","TM4",2015,6,19,128,"Link",null,{"$f":"520*0.0853","v":44.356000000000002},{"$f":"520*0.033","v":17.16},8.6319999999999997,"2015-06-10","2015-06-16","2015-06-22","2015-07-24","2015-07-27",12,70,70,40925.68,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.134611776E+20},40,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#31"},"2015-07-30",489000,"2016-06-30",17500,"2017-03-20",7900,"2018-03-23",4610,"2019-09-23",3600,"2019-04-29",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":2046.2840000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1964.43264},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,212,"Pail changed from 127 to 212","Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#31-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#12"},"UC",12,"LP","SIS",null,"ITW","TM1",2015,5,22,128,"Link",null,27.056999999999999,null,7.2910000000000004,"2015-04-28","2015-05-20","2015-05-23","2015-06-19","2015-06-30",15,10,9.8000000000000007,3686.34,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.22791088E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#12"},"2015-07-02",25100,"2015-08-04",5120,null,null,null,null,null,null,"2016-01-13",null,null,"2016-03-24",900,50,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":279},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":427.61544000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":280.16183999999998},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,125,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-UC#12-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#45"},"Ta",45,"HP","SIS",null,"ITE","TM4",2015,4,18,128,"Link",null,45.818100000000001,null,8.7739999999999991,"2015-04-01","2015-04-09","2015-04-18","2015-05-22","2015-06-01",11.1,65,65,31153.74,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.9535147679999997E+20},22.5,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#45"},"2015-06-06",218000,"2015-08-06",42900,"2016-06-30",13100,"2017-03-20",5720,"2018-03-23",3510,"2018-09-06",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1059.2271600000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":872.30472000000009},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,124,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#45-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#11"},"UC",11,"LP","SIS",null,"ITE","TM4",2014,11,25,127,"Link",null,25.713999999999999,5.0999999999999996,null,"2014-11-20","2014-11-22","2014-11-25","2014-12-21","2015-03-16",17.100000000000001,10,9.8000000000000007,4208.22,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.39274704E+19},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#11"},"2015-03-17",8570,"2015-08-04",1510,null,null,null,null,null,null,"2015-10-01",null,null,"2015-12-08",460,17,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":352},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":488.15352000000007},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":319.82472000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#11-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"ThO#1"},"ThO",1,"LP","SIS",null,"ITW","TM1",2014,11,15,127,"Link",null,25.518999999999998,11.083,7.274,"2014-11-05","2014-11-10","2014-11-14","2014-11-25","2015-03-09",12.1,10,9.8000000000000007,2053.85,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.5841931999999992E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"ThO#1"},"2015-03-13",6200,"2015-08-05",1440,null,null,null,null,null,null,"2016-01-13",null,null,"2016-03-24",1700,90,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":485},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1095},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":156.09259999999998},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,122,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-ThO#1-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#44"},"Ta",44,"HP","SIS",null,"ITE","TM4",2014,10,22,127,"Link",null,47.49,null,8.4860000000000007,"2014-09-24","2014-09-28","2014-10-01","2014-11-13","2014-11-18",11.8,70,60,38621.61,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.6203433519999982E+20},30,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#44"},"2014-11-21",276000,"2015-08-06",18000,"2016-06-30",8440,"2017-03-20",4370,null,null,"2017-10-26",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1313.1347400000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1081.40508},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,121,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#44-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"ZrC#6"},"ZrC",6,"LP","SIS",null,"ITW","TM1",2014,9,16,127,"Link",null,26.693000000000001,3.5139999999999998,7.3390000000000004,"2014-09-10","2014-09-14","2014-09-16","2014-09-29","2014-10-14",14.9,50,50,12307.84,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.747109888E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"ZrC#6"},"2014-10-21",112000,"2015-08-05",7380,"2016-06-29",2390,null,null,null,null,"2017-10-18",null,null,"2017-01-27",760,45,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":851},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":615.39200000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":443.08223999999996},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,120,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-ZrC#6-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#10"},"UC",10,"LP","SIS",null,"ITE","TM4",2014,8,20,126,"Link",null,29.207000000000001,2.2370000000000001,7.7450000000000001,"2014-08-11","2014-08-18","2014-08-20","2014-09-16","2014-09-23",14.5,10,9.8000000000000007,4842.41,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.080825912E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#10"},"2014-09-26",28900,"2015-08-04",1130,null,null,null,null,null,null,"2015-10-01",null,null,"2015-12-08",400,17,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":448},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":561.71956},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":368.02315999999996},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#10-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#43"},"Ta",43,"LP","SIS",null,"ITW","TM1",2014,7,28,126,"Link",null,45.92,null,7.3239999999999998,"2014-07-23","2014-07-25","2014-07-29","2014-08-20","2014-09-03",11.8,50,50,21279.51,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.7495866319999992E+20},22.5,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#43"},"2014-09-05",150000,"2015-08-05",5480,"2016-06-29",3470,null,null,null,null,"2016-10-18",null,null,"2017-01-27",1280,58,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":891},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":723.50333999999998},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":595.82628},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,118,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#43-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#30"},"SiC",30,"HP","FEBIAD",null,"ITE","TM3",2014,7,8,126,"Link",null,42.512999999999998,18.315000000000001,9.83,"2014-07-02","2014-07-05","2014-07-09","2014-07-26","2014-07-29",12.5,70,65,20093.43,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.4848535759999998E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#30"},"2015-08-06",211000,"2014-09-15",34100,"2015-08-05",6830,"2016-06-30",4700,"2017-03-20",2830,"2017-10-26",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1004.6715},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":964.48464000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,117,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM3-SiC#30-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#9"},"UC",9,"LP","SIS",null,"ITW","TM1",2014,6,18,126,"Link",null,28.074999999999999,null,7.3520000000000003,"2014-06-10","2014-06-13","2014-06-17","2014-07-06","2014-07-16",13.5,10,9.8000000000000007,1795.84,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.00831488E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#9"},"2014-07-21",7930,"2015-08-04",302,null,null,null,null,null,null,"2015-10-01",null,null,"2015-12-08",120,8,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":520},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":208.31744},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":136.48383999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-UC#9-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"TiC#4"},"TiC",4,"HP","SIS",null,"ITE","TM3",2014,5,20,126,"Link",null,21.99,4.42,8.609,"2014-05-06","2014-05-16","2014-05-20","2014-06-16","2014-06-24",12.7,100,98,40206.019999999997,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.973983663999999E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"TiC#4"},"2014-06-27",407000,"2015-08-05",7380,"2016-06-29",5120,"2017-03-20",3180,null,null,"2017-10-26",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1286.5926399999998},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1286.5926399999998},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,115,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM3-TiC#4-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#42"},"Ta",42,"LP","SIS",null,"ITW","TM4",2014,4,23,126,"Link",null,45.899000000000001,null,7.7140000000000004,"2014-04-02","2014-04-11","2014-04-16","2014-05-20","2014-05-27",12.5,50,50,25512.01,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.6942806319999989E+20},24.5,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#42"},"2014-05-30",277000,"2015-08-05",5170,"2016-06-28",3910,null,null,null,null,"2016-10-18",null,null,"2017-01-27",1170,40,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":983},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":867.40833999999995},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":714.33627999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,114,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM4-Ta#42-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#8"},"UC",8,"LP","IG-LIS",null,"ITE","TM4",2013,12,10,125,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-11262",22,3.452,8.32,"2013-12-05","2013-12-08","2013-12-10","2013-12-21","2014-01-20",14.3,10,9.8000000000000007,2228.09,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.97309688E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#8"},"2014-01-22",9200,"2014-05-13",1940,null,null,null,null,null,null,"2014-06-12",null,null,"2014-10-03",750,30,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":286},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":258.45844000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":169.33484000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#8-LP-IG-LIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#41"},"Ta",41,"HP","SIS",null,"ITW","TM4",2013,11,6,125,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-11261",42.19,null,8.6219999999999999,"2013-10-25","2013-10-29","2013-10-31","2013-12-02","2013-12-04",12.2,70,70,43123.93,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.6252611759999982E+20},22.5,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#41"},"2013-12-09",536000,"2014-05-16",37600,"2015-08-05",6590,"2016-06-28",5310,"2017-03-20",3680,"2017-10-26",null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1466.2136200000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1207.4700399999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,112,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM4-Ta#41-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"NiO#2"},"NiO",2,"HP","FEBIAD",null,"ITE","TM3",2013,10,9,125,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-11260",31.8,23.32,9.9429999999999996,"2013-10-07","2013-10-12","2013-10-17","2013-10-31","2013-11-19",9.1999999999999993,14,14,3934.9,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.7826967999999984E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"NiO#2"},"2013-11-22",76400,"2014-05-15",5310,null,null,null,null,null,null,"2014-11-26",null,null,"2015-03-13",1130,75,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":498},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":118.047},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":118.047},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM3-NiO#2-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#7"},"UC",7,"LP","SIS",null,"ITW","TM1",2013,9,13,125,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-11259",22,3.3380000000000001,7.3869999999999996,"2013-08-27","2013-09-10","2013-09-13","2013-10-07","2013-10-22",12.9,10,9.8000000000000007,3937.25,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.787942E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#7"},"2013-10-24",22600,"2014-05-13",1950,null,null,null,null,null,null,"2014-06-12",null,null,"2014-10-03",850,30,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":361},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":456.721},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":299.23099999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-UC#7-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#29"},"SiC",29,"HP","FEBIAD","CTL","ITE","TM4",2013,8,7,124,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9929",45.491999999999997,16.507999999999999,null,"2013-07-30","2013-08-04","2013-08-07","2013-08-14","2017-09-13",11.5,60,60,5396.52,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.204503264E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#29"},"2013-10-08",24700,"2014-05-14",3120,null,null,null,null,null,null,"2014-11-26",null,null,"2015-03-13",500,65,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":576},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":269.82600000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":259.03296},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#29-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#6"},"UC",6,"LP","SIS",null,"ITW","TM1",2013,7,10,124,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9928",22,null,null,"2013-07-02","2013-07-07","2013-07-11","2013-08-07","2013-08-27",16.2,10,9.8000000000000007,4591.97,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.024927704E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#6"},"2013-08-28",23100,"2014-05-13",1650,null,null,null,null,null,null,"2014-06-12",null,null,"2014-10-03",530,25,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":422},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":532.66852000000006},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":348.98972000000003},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-UC#6-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#40"},"Ta",40,"HP","SIS",null,"ITE","TM4",2013,6,6,124,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9927",null,null,null,"2013-05-28","2013-06-03","2013-06-05","2013-07-09","2013-07-23",11.5,70,70,39837.879999999997,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.8918148159999993E+20},51,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#40"},"2013-07-29",224000,"2014-05-16",15600,"2015-08-05",4930,"2016-06-29",4230,"2017-03-20",2740,"2017-05-02",null,null,"2017-07-07",1100,70,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1459},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1354.48792},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1115.46064},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,107,null,"Assayed",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#40-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#39"},"Ta",39,"LP","SIS",null,"ITW","TM1",2013,5,8,124,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9926",null,null,7.3079999999999998,"2013-04-09","2013-04-13","2013-05-07","2013-06-04","2013-06-25",12.8,45,45,24072.240000000002,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.372923968E+20},22.5,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#39"},"2013-07-02",95300,"2014-05-21",6100,"2014-09-12",4570,null,null,null,null,"2016-01-13",null,null,"2016-03-24",700,55,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1024},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":818.45616000000007},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":674.02272000000005},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#39-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#28"},"SiC",28,"LP","IG-LIS",null,"ITE","TM4",2013,4,18,124,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9771",38.479999999999997,null,8.4139999999999997,"2013-03-27","2013-04-15","2013-04-20","2013-05-07","2013-05-21",13.5,40,40,9538.36,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.128961952E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#28"},"2013-05-31",24800,"2014-05-14",1980,null,null,null,null,null,null,"2014-06-12",null,null,"2014-10-03",1000,40,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":514},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":476.91800000000006},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":457.84128000000004},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#28-LP-IG-LIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"TiC#3"},"TiC",3,"LP","SIS",null,"ITW","TM1",2012,11,26,123,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-8909",null,null,null,"2012-11-13","2012-11-23","2012-11-27","2012-12-21","2012-01-04",14.5,65,50,24082.39,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.3751894479999998E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"TiC#3"},"2013-01-15",98700,"2014-05-16",2510,null,null,null,null,null,null,"2014-11-26",null,null,"2015-03-13",560,30,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":812},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":770.63648000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":770.63648000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-TiC#3-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#5"},"UC",5,"LP","SIS",null,"ITE","TM4",2012,10,29,123,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-8908",null,null,null,"2012-10-23","2012-10-27","2012-10-31","2012-11-26","2012-12-04",14.6,10,9.8000000000000007,4874.2299999999996,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.0879281359999998E+20},48.9,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#5"},"2012-12-06",32600,"2013-06-20",2260,null,null,null,null,null,null,"2013-07-31",null,null,"2013-11-29",1100,35,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":368},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":565.41067999999996},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":370.44147999999996},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UC#5-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb#7"},"Nb",7,"LP","SIS",null,"ITW","TM1",2012,10,2,123,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-8907",26.529,null,null,"2012-09-25","2012-10-01","2012-10-03","2012-10-31","2012-11-06",12.1,40,40,23470.67,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.2386535439999998E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb#7"},"2012-11-09",178000,"2014-05-21",3500,null,null,null,null,null,null,"2014-11-26",null,null,"2015-03-13",1450,100,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":863},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":715.85543499999994},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":539.82540999999992},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Nb#7-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"NiO#1"},"NiO",1,"HP","FEBIAD",null,"ITE","TM4",2012,9,18,123,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-8718",null,null,null,"2012-09-10","2012-09-14","2012-09-26","2012-10-01","2012-10-09",12,16,20,1737.39,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.87785448E+19},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"NiO#1"},"2012-10-24",35500,"2013-06-20",1500,null,null,null,null,null,null,"2014-02-03",null,null,"2014-03-12",320,7,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":527},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":52.121700000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":52.121700000000004},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-NiO#1-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#4"},"UC",4,"LP","SIS",null,"ITW","TM1",2012,8,20,122,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-8648",null,null,null,"2012-08-14","2012-08-20","2012-08-23","2012-09-09","2016-09-14",13.9,10,9.8000000000000007,2994.25,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.683166E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#4"},"2012-09-14",55300,"2013-06-20",913,null,null,null,null,null,null,"2013-07-31",null,null,"2013-11-29",470,20,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":446},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":347.33300000000003},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":227.56299999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-UC#4-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UO2#3"},"UO2",3,"LP","FEBIAD",null,"ITE","TM4",2012,7,23,122,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-8597",null,null,null,"2012-07-09","2012-07-18","2012-07-24","2012-08-19","2016-09-05",12,10,9.8000000000000007,4654.25,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.0388286E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UO2#3"},"2012-09-07",42000,"2013-06-20",3860,null,null,null,null,null,null,"2013-07-31",null,null,"2014-03-12",1300,35,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":570},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":539.89300000000003},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":539.89300000000003},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-UO2#3-LP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#38"},"Ta",38,"LP","SIS",null,"ITW","TM1",2012,6,25,122,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-8541",42.8,null,null,"2012-06-19","2012-06-23","2012-06-26","2012-07-24","2012-07-31",12.7,40,40,20839.509999999998,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.6513786319999992E+20},22.5,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#38"},"2012-08-02",226000,"2014-05-21",2880,null,null,null,null,null,null,"2014-11-26",null,null,"2015-03-13",840,45,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":962},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":708.54333999999994},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":583.50627999999995},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#38-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#27"},"SiC",27,"HP","SIS",null,"ITE","TM4",2012,5,28,122,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-8530",null,null,null,"2012-05-22","2012-05-25","2012-05-28","2012-06-24","2012-07-03",12.3,75,70,29007.62,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.474500783999999E+20},53,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#27"},"2012-07-06",178000,"2014-05-15",3660,"2014-09-15",2700,null,null,null,null,"2016-01-13",null,null,"2016-03-24",1900,90,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1369},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1450.3810000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1392.3657599999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#27-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb#6"},"Nb",6,"LP","SIS",null,"ITW","TM1",2012,5,2,121,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-8190",24.52,null,null,"2012-04-24","2012-04-30","2012-05-02","2012-05-28","2012-06-05",12.6,40,40,21153.53,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.7214678959999995E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb#6"},"2012-06-11",152000,"2014-05-16",2120,null,null,null,null,null,null,"2014-06-12",null,null,"2014-10-03",1500,50,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":858},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":645.18266499999993},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":486.53118999999998},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Nb#6-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#3"},"UC",3,"LP","SIS",null,"ITW","TM1",2011,12,1,120,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7480",null,null,null,"2011-11-24","2011-11-29","2011-12-02","2011-12-21","2012-03-12",14.5,10,10,4171.8,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.3114576E+19},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#3"},"2012-03-03",11700,"2012-10-31",1890,null,null,null,null,null,null,"2013-07-31",null,null,"2013-11-29",166,10,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":709},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":483.92880000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":317.05680000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-UC#3-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#26"},"SiC",26,"HP","FEBIAD",null,"ITE","TM4",2011,11,10,120,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7312",null,null,null,"2011-11-04","2011-11-09","2011-11-10","2011-12-01","2012-05-14",11.6,70,75,33523.379999999997,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.4824184160000003E+20},36,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#26"},"2012-05-05",118000,"2014-05-16",4320,"2014-09-15",3650,"2015-08-04",2810,null,null,"2015-10-01",null,null,"2015-12-08",1650,65,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1468},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1676.1689999999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1609.1222399999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#26-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"TaC#1"},"TaC",1,"LP","SIS",null,"ITE","TM1",2011,10,9,120,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7311",null,null,null,"2011-10-04","2011-10-06","2011-10-08","2011-11-10","2011-11-14",12.6,55,55,33897.18,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.5658505759999984E+20},20,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"TaC#1"},"2011-11-16",239000,"2013-06-20",3550,null,null,null,null,null,null,"2014-02-03",null,null,"2014-03-12",1400,35,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":853},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":847.42950000000008},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":847.42950000000008},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM1-TaC#1-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#2"},"UC",2,"LP","SIS",null,"ITW","TM1",2011,9,1,119,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-6973",null,null,null,"2011-08-24","2011-08-29","2011-09-02","2011-09-26","2011-10-03",14.3,2,2,893.91,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.99520712E+19},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#2"},"2011-10-05",8910,"2011-12-12",1120,null,null,null,null,null,null,"2012-05-25",null,null,"2012-08-24",220,10,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":333},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":103.69356000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":67.937159999999992},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-UC#2-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#37"},"Ta",37,"LP","SIS",null,"ITW","TM1",2011,8,11,119,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-6861",null,null,null,"2011-08-03","2011-08-09","2011-08-12","2011-08-13","2011-08-17",14,40,40,484.67,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.08178344E+19},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#37"},"2011-09-14",840,"2011-11-08",470,null,null,null,null,null,null,"2012-01-05",null,null,"2012-02-29",160,10,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":200},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":16.47878},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":13.57076},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#37-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#36"},"Ta",36,"LP","SIS",null,"ITE","TM4",2011,7,27,119,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-6811",null,null,null,"2011-07-20","2011-07-22","2011-07-27","2011-09-01","2011-09-28",12.8,50,50,34831.550000000003,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.7744019599999998E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#36"},"2011-09-29",111000,"2013-06-20",4640,"2014-05-15",3260,"2014-09-15",2610,null,null,"2015-10-01",null,null,"2015-12-08",1100,36,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1559},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1184.2727000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":975.28340000000014},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#36-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#35"},"Ta",35,"HP","SIS",null,"ITE","TM4",2011,6,1,119,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-6503",null,null,null,"2011-05-26","2011-05-27","2011-05-31","2011-07-15","2011-07-19",11.3,70,70,58083.64,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.2964268447999997E+21},51,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#35"},"2011-07-25",411000,"2013-06-20",8260,"2014-05-21",4690,null,null,null,null,"2016-01-13",null,null,"2016-03-24",900,60,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1714},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1974.8437600000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1626.3419200000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#35-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#25"},"SiC",25,"HP","SIS",null,"ITE","TM4",2011,4,19,119,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-6241",null,null,null,"2011-01-10","2011-04-04","2011-04-16","2011-05-21","2011-05-25",11.4,68,68,16800.66,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.7499073119999997E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#25"},"2011-05-31",120000,"2012-10-31",4690,null,null,null,null,null,null,"2012-11-14",null,null,"2013-02-08",2000,80,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":629},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":840.03300000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":806.43168000000003},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#25-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UC#1"},"UC",1,"LP","SIS",null,"ITW","TM1",2010,12,5,118,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-5343",null,null,null,"2010-12-02","2010-12-05","2010-12-06","2010-12-22","2011-01-13",14.9,2,1.9,650.89,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.4527864799999998E+19},17,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UC#1"},"2011-01-14",1700,"2011-12-12",190,null,null,null,null,null,null,"2012-05-25",null,null,"2012-08-24",50,3,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":611},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":75.503240000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":49.467639999999996},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-UC#1-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb#5"},"Nb",5,"HP","SIS",null,"ITE","TM4",2010,10,31,118,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-5342",null,null,null,"2010-09-30","2010-10-26","2010-10-31","2010-12-03","2011-01-05",12.4,100,98,52597.32,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.1739721824000001E+21},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb#5"},"2011-01-11",230000,"2013-06-20",3050,null,null,null,null,null,null,"2014-02-03",null,null,"2014-03-12",1200,35,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1195},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1604.2182599999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1209.7383600000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Nb#5-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#24"},"SiC",24,"LP","SIS",null,"ITW","TM1",2010,10,1,118,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-5341",null,null,null,"2010-09-25","2010-09-28","2010-10-04","2010-10-18","2010-10-25",13.4,35,35,10015.42,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.2354417439999997E+20},40,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#24"},"2010-12-08",27000,"2011-11-08",1990,null,null,null,null,null,null,"2012-05-25",null,null,"2012-08-24",820,25,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":676},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":500.77100000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":480.74016},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-SiC#24-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#23"},"SiC",23,"HP","FEBIAD",null,"ITE","TM4",2010,9,1,117,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-5130",null,null,null,"2010-08-24","2010-08-27","2010-09-01","2010-09-22","2010-09-28",11.5,65,65,27130.639999999999,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.055558848E+20},36.6,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#23"},"2010-10-20",143000,"2013-06-20",3180,null,null,null,null,null,null,"2013-07-31",null,null,"2013-11-29",1600,55,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1164},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1356.5320000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1302.27072},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#23-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#33"},"Ta",33,"HP","SIS",null,"ITW","TM3",2010,8,6,117,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-5129",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":0},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#33"},null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM3-Ta#33-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#34"},"Ta",34,"LP","SIS",null,"ITW","TM1",2010,8,6,117,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-5181",null,null,null,"2010-07-31","2010-08-03","2010-08-05","2010-09-01","2010-09-23",13.7,45,45,24873.83,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.5518388560000011E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#34"},"2010-10-20",93000,"2011-12-14",4330,null,null,null,null,null,null,"2012-11-14",null,null,"2013-02-08",1600,60,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":891},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":845.71022000000016},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":696.46724000000006},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#34-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"ZrC#5"},"ZrC",5,"HP","FEBIAD",null,"ITE","TM4",2010,7,8,117,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-5048",null,null,null,"2010-06-22","2010-07-02","2010-07-08","2010-08-05","2010-08-19",11.3,75,75,36682.67,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.1875719439999998E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"ZrC#5"},"2010-08-25",292000,"2013-06-20",2650,null,null,null,null,null,null,"2014-02-03",null,null,"2014-03-12",1200,40,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1315},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1834.1334999999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1320.5761199999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-ZrC#5-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#22"},"SiC",22,"HP","SIS",null,"ITW","TM3",2010,6,12,117,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-4717",null,null,null,"2010-05-21","2010-06-11","2010-06-14","2010-06-30","2010-07-07",11.2,70,70,8013.64,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.788644448E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#22"},"2010-07-16",70100,"2011-12-14",1930,null,null,null,null,null,null,"2012-05-25",null,null,"2012-08-24",1000,40,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":786},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":400.68200000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":384.65472},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM3-SiC#22-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#30"},"Ta",30,"HP","SIS",null,"ITE","TM4",2010,4,27,117,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-4568",null,null,null,"2010-02-12","2010-02-17","N/A","N/A","2010-02-26","N/A","N/A","N/A",0,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":0},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#30"},null,null,null,null,null,null,null,null,null,null,"2010-06-10",null,null,"",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":0},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":0},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#30-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#32"},"Ta",32,"HP","SIS",null,"ITE","TM4",2010,4,27,117,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-4692",null,null,null,"2010-03-30","2010-04-18","2010-04-30","2010-06-02","2010-06-16",12.2,70,70,29214.97,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.5207813039999995E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#32"},"2010-07-16",124000,"2012-11-01",4790,null,null,null,null,null,null,"2012-11-14",null,null,"2013-02-08",2000,80,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":982},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":993.30898000000013},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":818.01916000000006},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#32-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#31"},"Ta",31,"HP","SIS",null,"ITW","TM3",2010,3,24,117,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-4606",null,null,null,"2010-03-18","2010-03-23","2010-03-24","2010-04-17","2010-05-07",11.3,70,70,25656.240000000002,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.726472768E+20},28,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#31"},"2010-06-06",116000,"2011-12-15",4170,null,null,null,null,null,null,"2012-11-14",null,null,"2013-02-08",2000,80,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1028},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":872.31216000000006},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":718.37472000000002},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM3-Ta#31-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UO2#2"},"UO2",2,"LP","FEBIAD",null,"ITW","TM3",2009,12,5,116,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-4409",null,null,null,"2009-11-30","2009-12-04","2009-12-06","2009-12-21","2010-01-19",5,2,2,426.29,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.5147928E+18},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UO2#2"},null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":49.449640000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":49.449640000000002},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM3-UO2#2-LP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb#4"},"Nb",4,"HP","SIS",null,"ITE","TM4",2009,10,21,116,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-4296",null,null,null,"2009-09-29","2009-10-19","2009-10-21","2009-11-24","2010-01-07",11.8,100,98,40805.07,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.1076916239999998E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb#4"},"2010-02-09",160000,"2011-11-10",3890,null,null,null,null,null,null,"2012-11-14",null,null,"2013-02-08",1300,50,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1172},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1244.554635},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":938.51661000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Nb#4-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#29"},"Ta",29,"HP","SIS",null,"ITE","TM4",2009,8,31,115,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-4145",null,null,null,"2009-08-26","2009-08-31","2009-09-01","2009-09-15","2009-09-25",11.8,70,70,14881.57,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.3215664240000002E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#29"},"2009-09-30",181000,"2011-12-12",1740,null,null,null,null,null,null,"2012-01-05",null,null,"2012-02-29",880,40,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":897},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":505.97338000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":416.68396000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#29-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#21"},"SiC",21,"LP","SIS",null,"ITW","TM1",2009,7,23,115,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-4039",null,null,null,"2009-07-08","2009-07-16","2009-07-24","2009-08-31","2009-09-17",12.5,35,40,10571.86,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.359639152E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#21"},"2010-01-14",11000,"2010-04-01",4580,null,1800,null,null,null,null,"2010-11-16",null,null,"2011-02-02",1000,45,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":520},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":528.59300000000007},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":507.44928000000004},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-SiC#21-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#28"},"Ta",28,"HP","SIS",null,"ITE","TM4",2009,6,25,115,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-4038",null,null,null,"2009-06-22","2009-06-26","2009-06-27","2009-07-22","2009-07-31",11.6,70,85,24445.81,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.4563047920000002E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#28"},"2009-08-07",159000,"2011-12-12",2440,null,null,null,null,null,null,"2012-01-05",null,null,"2012-02-29",1400,50,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":952},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":831.15754000000015},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":684.48268000000007},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Ta#28-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"ZrC#4"},"ZrC",4,"HP","FEBIAD",null,"ITW","TM3",2009,6,4,115,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-3980",null,null,null,"2009-09-18","2009-09-23","N/A","N/A","2009-10-02","N/A",75,"N/A",0,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":0},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"ZrC#4"},null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":0},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":0},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM3-ZrC#4-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#20"},"SiC",20,"HP","FEBIAD",null,"ITE","TM4",2009,5,8,115,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-4046",null,null,null,"2009-04-29","2009-05-04","2009-05-08","2009-05-31","2009-06-15",11.5,75,60,17246.04,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.849316128E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#20"},"2009-06-29",60700,"2010-04-01",8590,null,4000,null,null,null,null,"2010-11-16",null,null,"2011-02-02",4000,100,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":612},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":862.30200000000013},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":827.80992000000003},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#20-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#27"},"Ta",27,"LP","SIS",null,"ITW","TM1",2009,4,1,115,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-3790",null,null,null,"2009-02-13","2009-02-19","2009-04-01","2009-05-06","2009-05-20",11.7,35,40,28220.3,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.2987709599999997E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#27"},"2009-07-14",81000,"2011-12-14",2760,null,null,null,null,null,null,"2012-05-25",null,null,"2012-08-24",1500,60,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1206},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":959.49020000000007},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":790.16840000000002},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#27-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Al2O3#1"},"Al2O3",1,"HP","FEBIAD","CTL","ITE","TM4",2009,3,18,114,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-3789",null,null,null,"2009-03-06","2009-03-13","2009-03-21","2009-03-31","2009-04-15",8.1999999999999993,50,30,3174.57,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.08564024E+19},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Al2O3#1"},"2009-05-29",17200,"2010-04-07",2950,null,2430,null,null,null,null,"2010-07-14",null,null,"2010-09-14",1600,60,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":532},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-Al2O3#1-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#19"},"SiC",19,"LP","SIS",null,"ITW","TM1",2008,11,14,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-3559",null,null,null,"2008-11-14","2008-11-17","2008-11-20","2008-12-22","2009-01-23",14.1,40,50,23063.29,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.1477263280000002E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#19"},"2009-02-06",58600,"2009-03-24",23200,"2010-03-31",4100,null,null,null,null,"2010-07-14",null,null,"2010-09-14",1600,50,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":631},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1153.1645000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1107.03792},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-SiC#19-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#26"},"Ta",26,"HP","SIS",null,null,"TM4",2008,9,30,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-3563",null,null,null,"2008-09-30","2008-10-03","2008-10-07","2008-11-12","2009-01-30",10.9,70,70,40479.519999999997,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.0350288639999987E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#26"},"2009-02-06",131000,"2011-12-14",3370,null,null,null,null,null,null,"2012-01-05",null,null,"2012-02-29",1600,50,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1204},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1376.30368},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1133.4265599999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM4-Ta#26-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"UO2#1"},"UO2",1,null,null,null,null,"TM1",2008,8,21,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7658",null,null,null,"2008-08-21","2008-08-26","2008-08-29","2008-09-20","2008-10-07",10.8,2,2,295.17,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.5881944E+18},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"UO2#1"},"2008-11-04",971,null,null,null,null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":34.239720000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":34.239720000000005},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-UO2#1--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#25"},"Ta",25,"HP","SIS",null,null,"TM4",2008,7,8,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-3565",null,null,null,"2008-07-08","2008-07-12","2008-07-17","2008-08-21","2008-09-26",11.1,75,100,46076.02,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.0284167663999999E+21},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#25"},"2008-10-02",225000,"2011-11-10",4570,null,4570,null,null,null,null,"2012-01-05",null,null,"2012-02-29",2700,90,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1287},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1566.5846799999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1290.1285599999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM4-Ta#25-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#18"},"SiC",18,"LP","SIS",null,"ITW","TM2",2008,6,3,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7659",null,null,null,"2008-06-03","2008-06-17","2008-06-20","2008-07-07","2008-07-16",14.2,40,45,6067.89,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.354353048E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#18"},"2008-07-24",25200,"2009-03-27",3200,null,3200,null,null,null,null,"2009-07-23",null,null,"2010-01-08",600,30,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":550},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":303.39450000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":291.25872000000004},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM2-SiC#18-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#17"},"SiC",17,"HP","FEBIAD",null,"ITE","TM4",2008,4,29,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7654",null,null,null,"2008-04-29","2008-05-13","2008-05-15","2008-06-17","2008-06-23",11.5,70,70,32349.119999999999,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.2203235839999987E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#17"},"2008-07-10",110000,"2010-04-07",5200,null,3500,null,null,null,null,"2010-11-16",null,null,"2011-02-02",1600,95,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":960},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1617.4560000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1552.75776},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#17-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#24"},"Ta",24,"LP","SIS",null,"ITW","TM1",2008,4,3,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7657",null,null,null,"2008-04-03","2008-04-10","2008-04-11","2008-05-07","2008-05-14",13.7,60,55,14440.79,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.2231843279999998E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#24"},"2008-06-19",49500,"2010-04-01",2800,null,null,null,null,null,null,"2010-07-14",null,null,"2010-09-14",920,35,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":860},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":490.98686000000009},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":404.34212000000002},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#24-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#23"},"Ta",23,"HP","SIS",null,null,"TM2",2007,11,24,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-2548",null,null,null,"2007-11-14","2007-11-19","2007-11-21","2007-12-21","2008-02-05",11.7,75,75,37697.93,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.4141779759999995E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#23"},"2008-02-21",149000,"2010-04-07",6640,null,4000,null,null,null,null,"2010-11-16",null,null,"2011-02-02",2700,75,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1139},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1281.7296200000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1055.54204},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM2-Ta#23-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#16"},"SiC",16,"HP","FEBIAD",null,null,"TM4",2007,10,24,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7652",null,null,null,"2007-10-24","2007-10-29","2007-11-01","2007-11-21","2008-02-12",11.2,75,75,13238.65,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.9548666799999995E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#16"},"2008-02-21",30000,"2009-03-25",3700,null,3700,null,null,null,null,"2009-07-23",null,null,"2010-01-08",1200,45,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":779},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":661.9325},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":635.45519999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM4-SiC#16-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#15"},"SiC",15,null,"SIS",null,null,"TM1",2007,9,18,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7655",null,null,null,"2007-09-18","2007-09-28","2007-10-05","2007-10-31","2007-11-08",14.5,40,40,17576.71,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.9231216719999998E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#15"},null,null,null,null,null,3500,null,null,null,null,"2009-05-19",null,null,"2009-08-28",930,35,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":667},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":878.83550000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":843.68207999999993},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-SiC#15--SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#22"},"Ta",22,"HP","SIS",null,null,"TM4",2007,7,18,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7653",null,null,null,"2007-07-18","2007-07-26","2007-07-27","2007-09-01","2007-09-07",11.5,85,80,33636.769999999997,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.5077270639999989E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#22"},"2007-09-12",234000,"2009-03-25",9000,"2010-03-31",4100,null,null,null,null,"2010-07-14",null,null,"2010-09-14",1800,65,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1109},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1143.6501799999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":941.8295599999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM4-Ta#22-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#21"},"Ta",21,"HP","SIS",null,null,"TM2",2007,6,26,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-3741",null,null,null,"2007-06-26","2007-06-30","2007-07-02","2007-07-26","2007-08-29",11.2,85,70,21527.4,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.80491568E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#21"},"2007-09-12",140000,"2009-03-25",7800,null,3475,null,null,null,null,"2010-07-14",null,null,"2010-09-14",1400,55,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1146},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":731.93160000000012},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":602.7672},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM2-Ta#21-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#14"},"SiC",14,"HP","FEBIAD",null,null,"TM4",2007,5,30,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7651",null,null,null,"2007-05-30","2007-06-13","2007-06-15","2007-06-29","2007-07-13",12,75,70,8897.18,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.985850576E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#14"},null,null,null,null,null,2500,null,null,null,null,"2009-05-19",null,null,"2009-08-28",650,23,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":791},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":444.85900000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":427.06464},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM4-SiC#14-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#20"},"Ta",20,"HP","SIS",null,null,"TM2",2007,4,12,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7656",null,null,null,"2007-04-12","2007-04-29","2007-05-01","2007-06-10","2007-06-18",11.6,70,80,42282.73,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.4375053359999995E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#20"},"2007-06-29",268000,"2009-03-24",10000,null,4000,null,null,null,null,"2010-11-16",null,null,"2011-02-02",2700,75,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1333},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1437.6128200000003},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1183.9164400000002},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM2-Ta#20-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#19"},"Ta",19,"LP","SIS",null,"ITW","TM1",2006,11,16,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7660",null,null,null,"2006-11-16","2006-12-14","2006-12-19","2007-01-20","2007-02-09",13.3,50,50,17370.240000000002,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.877037568E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#19"},null,null,null,null,null,4100,null,null,null,null,"2009-05-19",null,null,"2009-08-28",1250,32,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":951},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":590.58816000000013},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":486.36672000000004},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#19-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"TiC#2"},"TiC",2,"HP","FEBIAD",null,"ITE","TM4",2006,11,3,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7661",null,null,null,"2006-11-03","2006-11-10","2006-11-17","2006-12-14","2007-03-13",10.7,75,70,17577.439999999999,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.9232846079999993E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"TiC#2"},null,null,null,null,null,2700,null,null,null,null,"2009-05-19",null,null,"2009-08-28",700,30,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":988},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":562.47807999999998},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":562.47807999999998},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-TiC#2-HP-FEBIAD"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#18"},"Ta",18,"LP","SIS",null,"ITW","TM1",2006,9,27,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7644",null,null,null,"2006-09-27","2006-10-03","2006-10-07","2006-11-01","2006-11-14",13.6,50,35,15658.22,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.4949147039999997E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#18"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2009-01-09",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":800},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":532.37948000000006},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":438.43016},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#18-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb5SiC3#1"},"Nb5SiC3",1,"LP","SIS",null,"ITW","TM1",2006,8,15,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7641",null,null,null,"2006-08-15","2006-08-30","2006-08-31","2006-09-20","2006-09-25",12.8,30,20,3582.23,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.9955373599999984E+19},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb5SiC3#1"},null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Nb5SiC3#1-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#13"},"SiC",13,"HP","SIS",null,"ITE","TM2",2006,7,6,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7638",null,null,null,"2006-07-05","2006-07-21","2006-07-26","2006-08-30","2006-11-02",12.2,70,65,22905.05,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.1124071599999995E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#13"},"2007-02-05",33700,"2009-03-27",4000,null,4000,null,null,null,null,"2009-07-23",null,null,"2010-01-08",1150,60,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1227},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1145.2525000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1099.4423999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM2-SiC#13-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#17"},"Ta",17,"LP","SIS",null,"ITW","TM1",2006,6,6,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7643",null,null,null,"2006-06-06","2006-06-13","2006-06-16","2006-07-26","2006-08-02",12.9,55,40,25761.71,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.7500136719999998E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#17"},null,null,null,null,null,3800,null,null,null,null,"2009-05-19",null,null,"2009-08-28",1450,46,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1129},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":875.89814000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":721.32787999999994},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#17-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#16"},"Ta",16,"HP","SIS",null,"ITE","TM2",2006,4,25,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7640",null,null,null,"2006-04-25","2006-05-08","2006-05-11","2006-06-13","2006-06-28",12.9,55,100,38923.199999999997,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.6876582399999987E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#16"},"2006-07-18",170,"2009-03-27",5900,null,5900,null,null,null,null,"2009-07-28",null,null,"2010-01-08",1900,85,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1305},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1323.3887999999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1089.8496},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM2-Ta#16-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#15"},"Ta",15,"LP","SIS",null,"ITW","TM1",2006,3,28,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7642",null,null,null,"2006-03-28","2006-04-01","2006-04-05","2006-05-09","2006-05-17",13.2,45,35,19354.599999999999,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.3199467199999993E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#15"},null,null,null,null,null,3800,null,null,null,null,null,null,null,"2007-10-05",1720,170,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":514},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":658.05640000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":541.92880000000002},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#15-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#14"},"Ta",14,"HP","SIS",null,"ITE","TM2",2006,2,21,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-7639",null,null,null,"2006-02-21","2006-03-06","2006-03-13","2006-04-01","2006-04-19",12.1,65,65,14745.51,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.2911978319999992E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#14"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2009-01-09",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1014},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":501.34734000000003},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":412.87428},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM2-Ta#14-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"ZrC#3"},"ZrC",3,"LP","SIS",null,"ITW","TM1",2005,11,18,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-1183",null,null,null,"2005-11-18","2005-11-23","2005-11-28","2005-12-21","2006-02-03",13.3,40,40,10669.91,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.3815239119999998E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"ZrC#3"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2009-01-09",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1115},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":533.49549999999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":384.11675999999994},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-ZrC#3-LP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#12"},"SiC",12,"HP","SIS",null,null,"TM2",2005,9,29,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-1179",null,null,null,"2005-09-29","2005-10-04","2005-10-06","2005-11-02","2005-11-07",11.4,70,70,31816.07,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.1013468239999992E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#12"},"2005-11-10",440000,"34/03/2009",4250,null,4250,null,null,null,null,"2009-07-23",null,null,"2010-01-08",1400,65,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1528},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1590.8035},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1527.17136},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM2-SiC#12-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#13"},"Ta",13,"HP",null,null,null,"TM2",2005,8,9,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-1189",null,null,null,"2005-08-09","2005-08-24","2005-08-25","2005-09-06","2005-09-14",11.4,65,55,11152.25,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.4891821999999998E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#13"},null,null,null,null,null,2305,null,null,null,null,null,null,null,"2007-10-05",1400,90,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":759},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":379.17650000000003},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":312.26300000000003},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM2-Ta#13-HP-"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#12"},"Ta",12,null,null,null,"ITW","TM1",2005,7,20,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-1192",null,null,null,"2005-07-20","2005-07-25","2005-07-28","2005-09-20","2005-09-22",13.3,35,35,22903.34,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.1120254879999997E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#12"},null,null,null,null,null,3525,null,null,null,null,null,null,null,"2007-10-05",1910,109,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":745},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":778.71356000000003},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":641.29352000000006},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITW-TM1-Ta#12--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#11"},"SiC",11,"HP","SIS",null,null,"TM2",2005,6,8,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-1181",null,null,null,"2005-06-08","2005-06-13","2005-06-15","2005-07-12","2005-07-19",12.9,65,65,29202.240000000002,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.517939968E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#11"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2009-01-09",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1277},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":1460.1120000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":1401.7075200000002},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM2-SiC#11-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"CaZrO3#3"},"CaZrO3",3,null,"ECR",null,"ITE","TM3",2005,5,18,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-1172",null,null,null,"2005-05-18","2005-05-26","2005-05-27","2005-06-13","2005-08-03",12.6,3,2,476.63,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.06383816E+19},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"CaZrO3#3"},null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM3-CaZrO3#3--ECR"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#11"},"Ta",11,null,null,null,null,"TM1",2005,3,10,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-1190",null,null,null,"2005-03-10","2005-03-29","2005-03-31","2005-05-25","2005-05-31",12.9,40,40,14363.39,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.2059086479999992E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#11"},null,null,null,null,null,2098,null,null,null,null,null,null,null,"2007-10-05",770,74,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":863},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":488.35525999999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":402.17491999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Ta#11--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#10"},"SiC",10,"HP",null,null,null,"TM2",2005,3,3,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-1178",null,null,null,"2005-03-03","2005-04-12","2005-04-22","2005-05-03","2005-05-17",12.4,40,65,6995.03,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.5612906959999998E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#10"},null,null,null,null,null,1450,null,null,null,null,null,null,null,"2007-04-20",480,35,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":717},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":349.75150000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":335.76143999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM2-SiC#10-HP-"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"ZrC#2"},"ZrC",2,null,"SIS",null,null,"TM1",2004,11,1,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-1185",null,null,null,"2004-12-02","2004-12-09","2004-12-07","2004-12-20","2005-02-02",14,35,35,4264.54,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":9.5184532799999984E+19},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"ZrC#2"},null,null,null,null,null,570,null,null,null,null,null,null,null,"2007-04-20",350,20,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":851},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":213.227},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":153.52343999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-ZrC#2--SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#10"},"Ta",10,null,null,null,null,"TM1",2004,9,21,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2004-09-21","2004-09-26","2004-10-13","2004-11-14","2004-11-18",12.6,40,40,17207.37,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.8406849840000002E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#10"},null,null,null,null,null,2500,null,null,null,null,null,null,null,"2007-04-20",900,35,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":887},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":585.05057999999997},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":481.80635999999998},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Ta#10--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#9"},"Ta",9,"HP",null,null,null,"TM2",2004,8,18,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-1188",null,null,null,"2004-08-18","2004-09-08","2004-09-10","2004-10-13","2004-10-27",11.6,70,70,10082.24,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.2503559679999997E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#9"},null,null,null,null,null,1070,null,null,null,null,null,null,null,"2007-04-20",480,17,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":919},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":342.79616000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":282.30272000000002},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM2-Ta#9-HP-"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#8"},"Ta",8,null,null,null,null,"TM1",2004,7,13,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-3740",null,null,null,"2004-07-13","2004-07-18","2004-07-26","2004-09-08","2004-09-15",12.6,40,40,22218.31,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.9591267919999998E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#8"},null,null,null,null,null,4400,null,null,null,null,null,null,null,"2006-03-16",1250,80,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":554},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":755.42254000000014},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":622.11268000000007},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Ta#8--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#9"},"SiC",9,null,null,null,null,"TM2",2004,6,17,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2004-06-17","2004-06-28","2004-07-01","2004-07-22","2004-08-11",13.1,35,35,11767.73,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.6265573360000002E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#9"},null,null,null,null,null,1600,null,null,null,null,null,null,null,"2006-03-16",740,30,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":602},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":588.38649999999996},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":564.85104000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM2-SiC#9--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#8"},"SiC",8,null,null,null,null,"TM1",2004,5,7,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2004-05-07","2004-05-12","2004-05-14","2004-06-30","2004-07-08","?",35,35,15579.55,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.4773555599999992E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#8"},null,null,null,null,null,2750,null,null,null,null,null,null,null,"2006-03-16",1200,50,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":624},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":778.97749999999996},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":747.8184},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-SiC#8--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#7"},"SiC",7,null,"ECR",null,null,"TM3",2004,4,20,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2004-04-20","2004-04-27","2004-04-29","2004-06-08","2004-06-17","?",30,30,6247.31,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.394399592E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#7"},null,null,null,null,null,550,null,null,null,null,null,null,null,"2007-04-20",123,10,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1046},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":312.36550000000005},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":299.87088},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM3-SiC#7--ECR"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#7"},"Ta",7,null,null,null,null,"TM1",2004,3,9,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-3739",null,null,null,"2004-03-09","2004-03-15","2004-03-17","2004-04-25","2004-04-28","?",40,40,20159.5,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.4996003999999997E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#7"},null,null,null,null,null,4200,null,null,null,null,null,null,null,"2006-03-16",1200,73,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":690},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":685.423},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":564.46600000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Ta#7--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#6"},"SiC",6,null,null,null,null,"TM1",2003,11,6,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2003-11-06","2003-11-10","2003-11-13","2003-12-19","2004-01-16","?",30,30,14139,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.1558248E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#6"},null,null,null,null,null,2000,null,null,null,null,null,null,null,"2006-03-16",900,37,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":818},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":706.95},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":678.67200000000003},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-SiC#6--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#6"},"Ta",6,null,null,null,null,"TM1",2003,10,1,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-3737",null,null,null,"2003-09-25","2003-10-01","2003-10-05","2003-10-27","2003-11-03","?",40,40,13888.01,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.0998038320000002E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#6"},null,null,null,null,null,2200,null,null,null,null,null,null,null,"2006-03-16",950,35,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":871},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":472.19234000000006},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":388.86428000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Ta#6--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#5"},"Ta",5,null,null,null,null,"TM2",2003,6,24,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2003-06-24","2003-07-06","2003-07-21","2003-09-03","2003-10-28","?",40,40,23000.69,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":5.1337540079999995E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#5"},null,null,null,null,null,3250,null,null,null,null,null,null,null,"2006-03-16",1600,65,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":925},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":782.02346},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":644.01931999999999},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM2-Ta#5--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#5"},"SiC",5,null,null,null,null,"TM1",2003,5,26,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2003-05-26","2003-05-30","2003-06-02","2003-07-15","2003-07-30","?",30,30,14482.6,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.23251632E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#5"},null,null,null,null,null,1300,null,null,null,null,null,null,null,"2007-04-20",370,21,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1375},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":724.13000000000011},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":695.16480000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-SiC#5--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#4"},"Ta",4,null,"ECR",null,null,"TM3",2003,4,4,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2003-10-30","2003-11-08","N/A","N/A","2004-01-05","?",45,45,0,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":0},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#4"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2007-04-20",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#VALUE!"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":0},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":0},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM3-Ta#4--ECR"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"ZrC#1"},"ZrC",1,null,null,null,null,"TM1",2003,2,28,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2003-02-28","2003-03-11","2003-03-18","2003-04-28","2003-05-16","?",45,45,17668.96,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.9437118719999993E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"ZrC#1"},null,null,null,null,null,475,null,null,null,null,null,null,null,"2007-10-05",225,24,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1621},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":883.44799999999998},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":636.08255999999994},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-ZrC#1--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#4"},"SiC",4,null,null,null,null,"TM1",2002,11,2,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9431",null,null,null,"2002-11-01","2002-11-05","2002-11-10","2002-12-19","2003-01-17","?",45,45,19476.75,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.3472105999999998E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#4"},null,null,null,null,null,1200,null,null,null,null,null,null,null,"2007-04-20",240,14,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1583},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":973.83750000000009},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":934.88400000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-SiC#4--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"TiC#1"},"TiC",1,null,null,null,null,"TM1",2002,8,27,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9425",null,null,null,"2002-08-26","2002-08-29","2002-09-06","2002-10-23","2002-10-29","?",40,40,22265.9,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.9697488799999997E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"TiC#1"},null,null,null,null,null,560,null,null,null,null,null,null,null,"2007-04-20",240,7,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1640},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":712.50880000000006},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":712.50880000000006},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-TiC#1--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#3"},"Ta",3,null,null,null,null,"TM1",2002,6,8,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9427",null,null,null,"2002-05-30","2002-06-05","2002-07-07","2002-08-14","2002-08-21","?",20,20,27368.5,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":6.1086492000000003E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#3"},null,null,null,null,null,2750,null,null,null,null,null,null,null,"2006-03-16",1300,45,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1310},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":930.52900000000011},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":766.31799999999998},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Ta#3--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#3"},"SiC",3,null,null,null,null,"TM1",2002,3,16,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9433",null,null,null,"2002-03-13","2002-03-21","2002-04-13","2002-05-22","2002-05-28","?",45,45,7884.8,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.75988736E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#3"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2005-07-20",1100,200,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1155},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":394.24},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":378.47040000000004},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-SiC#3--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#2"},"SiC",2,null,null,null,null,"TM1",2001,9,18,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9435",null,null,null,"2001-09-25","2001-09-27","2001-10-03","2001-12-19","2002-02-26","?",15,15,16126.7,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.5994794399999997E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#2"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2005-07-20",1000,40,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1309},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":806.33500000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":774.08160000000009},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-SiC#2--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#2"},"Ta",2,null,null,null,null,"TM1",2001,6,8,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9429",null,null,null,"2001-07-07","2001-07-12","2001-07-16","2001-09-06","2001-09-11","?",40,40,17287,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":3.8584584E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#2"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2005-07-20",1200,55,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1413},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":587.75800000000004},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":484.036},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Ta#2--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb#3"},"Nb",3,null,null,null,null,"TM1",2001,4,13,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9420",null,null,null,"2001-04-12","2001-04-24","2001-04-27","2001-05-26","2001-05-30","?",40,40,3765.33,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.4042165599999984E+19},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb#3"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2007-04-20",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":2155},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":114.84256499999999},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":86.602589999999992},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Nb#3--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#1"},"SiC",1,null,null,null,null,"TM1",2000,11,18,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9422",null,null,null,"2000-11-17","2000-11-21","2000-11-22","2000-12-20","2001-04-09","?",10,10,2155,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":4.80996E+19},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#1"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2007-04-20",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":2312},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":107.75},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":103.44},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-SiC#1--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"CaZrO3#1"},"CaZrO3",1,null,null,null,null,"TM1",2000,6,24,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":"Link"},"https://documents.triumf.ca/docushare/dsweb/View/Collection-9417",null,null,null,"?","2000-09-28","2000-10-05","2000-11-11","2000-11-16","?",3,3,1338.24,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.98695168E+19},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"CaZrO3#1"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2007-04-20",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":2351},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-CaZrO3#1--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Ta#1"},"Ta",1,null,null,null,null,"TM1",2000,6,10,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2000-06-09","2000-06-14","2000-06-18","2000-07-15","2000-07-19","?",20,20,3515.83,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":7.84733256E+19},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Ta#1"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2005-07-20",95,5,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1831},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":119.53822000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":98.443240000000003},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Ta#1--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb#2"},"Nb",2,null,null,null,null,"TM1",1999,11,1,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"2000-03-17","2000-04-14","2000-04-18","2000-06-04","2000-06-07","?",10,10,9062.7999999999993,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.0228169599999997E+20},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb#2"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2005-07-20",85,5,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":1872},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":276.41539999999998},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":208.44439999999997},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Nb#2--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"Nb#1"},"Nb",1,null,null,null,null,"TM1",1999,6,14,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"1999-07-13","1999-07-15","1999-07-22","1999-08-20","1999-10-20","?",10,10,967,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":2.1583439999999996E+19},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"Nb#1"},null,null,null,null,null,null,null,null,null,null,null,null,null,"2007-04-20",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":2800},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":29.493500000000001},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":22.241},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-Nb#1--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"CaO#2"},"CaO",2,null,null,null,null,"TM1",1998,12,20,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"1999-04-09","1999-04-13","1999-04-15","1999-05-14","1999-05-27","?",1,1,363,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.10216E+18},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"CaO#2"},null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-CaO#2--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"CaO#1"},"CaO",1,null,null,null,null,"TM1",1998,11,25,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,null,null,"1998-11-22","1998-11-25","1998-11-30","1998-12-06","1998-12-10","?",1,1,37,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":8.2584E+17},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"CaO#1"},null,null,null,null,null,null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,null,null,null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"-TM1-CaO#1--"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"SiC#41"},"SiC",41,"HP","SIS",null,"ITE","TM4",null,null,null,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,{"$f":"29.049-22.009","v":7.0399999999999991},null,"2021-09-15","2021-09-16","2021-09-19","2021-09-27","2021-10-04",12.4,75,95,6004.5,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":1.3402044E+20},44,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"SiC#41"},"13/10/2021",33100,"2022-01-30",7800,"2022-12-16",{"$f":"1.46*1000","v":1460},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":300.22500000000002},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":288.21600000000001},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},"5B",260,"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope.","Measured",{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"ITE-TM4-SiC#41-HP-SIS"}]
[{"$f":"_xlfn.CONCAT(Table1[[#This Row],[Material]],\"#\",Table1[[#This Row],[No]])","v":"2A3M20#"},"2A3M20",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Table1[[#This Row],[URL]]=\"\",\"\",HYPERLINK(Table1[[#This Row],[URL]],\"Link\"))","v":""},null,null,{"$f":"29.049-22.009","v":7.0399999999999991},null,null,null,null,null,null,null,null,null,null,{"$f":"Table1[[#This Row],[Net Charge \n'[uAh']]]*6200000000000000000*0.000001*3600","v":0},null,{"$f":"CONCATENATE(Table1[[#This Row],[Material]], \"#\", Table1[[#This Row],[No]])","v":"2A3M20#"},"2021-06-10",235,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AND(AND(Table1[[#This Row],[Online p+]]>0,Table1[[#This Row],[Shipping Date]]>0),NOT(Table1[[#This Row],[Shipping Date]]=\"\")),Table1[[#This Row],[Shipping Date]]-Table1[[#This Row],[Offline p+]], NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.034,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.05,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.0305,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",1095,TRUE,NA()),NA())","v":{"$error":"#N/A"}},{"$f":"IF(Table1[[#This Row],[Offline p+]]>0,_xlfn.IFS(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.028,Table1[[#This Row],[Material]]=\"ZrC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.036,Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.116,Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.048,Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.032,Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.03,Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.023,Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.025,Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Net Charge \n'[uAh']]]*0.076,TRUE,NA()),NA())","v":{"$error":"#N/A"}},null,null,null,{"$f":"IF(Table1[[#This Row],[Schedule end]]>0,IF(Table1[[#This Row],[Material]]=\"Ta\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.028,IF(Table1[[#This Row],[Material]]=\"ZrC\",\nTable1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.036,IF(Table1[[#This Row],[Material]]=\"UO2\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.116,IF(Table1[[#This Row],[Material]]=\"UC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"SiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,IF(Table1[[#This Row],[Material]]=\"nSiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.048,IF(Table1[[#This Row],[Material]]=\"TiC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.032,IF(Table1[[#This Row],[Material]]=\"NiO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.03,IF(Table1[[#This Row],[Material]]=\"Nb\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.023,IF(Table1[[#This Row],[Material]]=\"TaC\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.025,IF(Table1[[#This Row],[Material]]=\"ThO\",Table1[[#This Row],[Estimated current]]*(Table1[[#This Row],[Schedule end]]-Table1[[#This Row],[Schedule start]])*24*0.076,NA()))))))))))),NA())","v":{"$error":"#N/A"}},{"$f":"Table1[[#This Row],[Estimated ship days]]/365","v":{"$error":"#N/A"}},null,252,"Contains 2A3M20, TM4 wiring, other little metal bits.",null,{"$f":"Table1[[#This Row],[TS]]&\"-\"&Table1[[#This Row],[TM]]&\"-\"&Table1[[#This Row],[Material]]&\"#\"&Table1[[#This Row],[No]]&\"-\"&Table1[[#This Row],[HP/LP]]&\"-\"&Table1[[#This Row],[IS]]","v":"--2A3M20#--"}]
[]
[]
[]
[]
[null,null,null,null,{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(Vault!A15,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],71)>0, \" \",INDEX(Table1[Target ID],MATCH(Vault!A15,Table1[Vault location],0))))","v":" "}]

{"sheet":"TargetOrder","index":1,"n_rows":15,"n_cols":13,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Year",null,null,null,2021]
[]
["Target","Year","Month","Day","Date","HP/LP","IS","Note","TM","-> HC","->TS","Target Oven","Heat Shield"]
[{"$f":"IFERROR(INDEX('Target Index'!A4:A197,SMALL(IF($E$1=Table1[Year],ROW('Target Index'!A4:A197)- MIN(ROW('Target Index'!A4:A197))+1,\"\"), ROW()-3)),\"\")","v":"UC#35"},{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A4,Table1[ID],0)),\"\")","v":2021},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A4,Table1[ID],0)),\"\")","v":11},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A4,Table1[ID],0)),\"\")","v":26},{"$f":"IFERROR(DATE(B4,C4,D4),\"\")","v":"2021-11-26"},{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A4,Table1[ID],0)),\"\")","v":"LP"},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A4,Table1[ID],0)),\"\")","v":"IG-LIS"},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A4,Table1[ID],0)),\"\")","v":0},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A4,Table1[ID],0)),\"\")","v":"TM4"},"2021-08-31",{"$f":"IF(J4>0,J4-7,\"\")","v":"2021-08-24"}]
["C#3",{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A5,Table1[ID],0)),\"\")","v":2021},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A5,Table1[ID],0)),\"\")","v":11},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A5,Table1[ID],0)),\"\")","v":5},{"$f":"IFERROR(DATE(B5,C5,D5),\"\")","v":"2021-11-05"},{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A5,Table1[ID],0)),\"\")","v":"LP"},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A5,Table1[ID],0)),\"\")","v":"SIS"},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A5,Table1[ID],0)),\"\")","v":0},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A5,Table1[ID],0)),\"\")","v":"TM2"},"2021-08-04",{"$f":"IF(J5>0,J5-7,\"\")","v":"2021-07-28"}]
["SiC#40",{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A6,Table1[ID],0)),\"\")","v":2021},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A6,Table1[ID],0)),\"\")","v":9},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A6,Table1[ID],0)),\"\")","v":14},"2021-09-14",{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A6,Table1[ID],0)),\"\")","v":"HP"},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A6,Table1[ID],0)),\"\")","v":"SIS"},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A6,Table1[ID],0)),\"\")","v":0},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A6,Table1[ID],0)),\"\")","v":"TM4"},"2021-07-06","2021-06-29"]
["UC#34",{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A7,Table1[ID],0)),\"\")","v":2021},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A7,Table1[ID],0)),\"\")","v":8},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A7,Table1[ID],0)),\"\")","v":25},"2021-08-25",{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A7,Table1[ID],0)),\"\")","v":"LP"},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A7,Table1[ID],0)),\"\")","v":"SIS"},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A7,Table1[ID],0)),\"\")","v":0},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A7,Table1[ID],0)),\"\")","v":"TM2"},"2021-06-10","2021-06-03"]
["Ta#62",{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A8,Table1[ID],0)),\"\")","v":2021},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A8,Table1[ID],0)),\"\")","v":7},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A8,Table1[ID],0)),\"\")","v":28},"2021-07-28",{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A8,Table1[ID],0)),\"\")","v":"LP"},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A8,Table1[ID],0)),\"\")","v":"SIS"},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A8,Table1[ID],0)),\"\")","v":0},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A8,Table1[ID],0)),\"\")","v":"TM4"},"2021-06-01","2021-05-25"]
["UC#33",{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A9,Table1[ID],0)),\"\")","v":2021},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A9,Table1[ID],0)),\"\")","v":6},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A9,Table1[ID],0)),\"\")","v":29},"2021-06-29",{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A9,Table1[ID],0)),\"\")","v":"LP"},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A9,Table1[ID],0)),\"\")","v":"SIS"},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A9,Table1[ID],0)),\"\")","v":0},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A9,Table1[ID],0)),\"\")","v":"TM2"},null,""]
["UC#32",{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A10,Table1[ID],0)),\"\")","v":2021},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A10,Table1[ID],0)),\"\")","v":6},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A10,Table1[ID],0)),\"\")","v":16},"2021-06-16",{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A10,Table1[ID],0)),\"\")","v":"P2N"},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A10,Table1[ID],0)),\"\")","v":"SIS"},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A10,Table1[ID],0)),\"\")","v":0},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A10,Table1[ID],0)),\"\")","v":"TM4"},null,""]
["",{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A11,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A11,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A11,Table1[ID],0)),\"\")","v":""},"",{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A11,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A11,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A11,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A11,Table1[ID],0)),\"\")","v":""},null,""]
["",{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A12,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A12,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A12,Table1[ID],0)),\"\")","v":""},"",{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A12,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A12,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A12,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A12,Table1[ID],0)),\"\")","v":""},null,""]
["",{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A13,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A13,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A13,Table1[ID],0)),\"\")","v":""},"",{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A13,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A13,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A13,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A13,Table1[ID],0)),\"\")","v":""},null,""]
["",{"$f":"_xlfn.IFNA(INDEX(Table1[Year],MATCH($A14,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Month],MATCH($A14,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Day],MATCH($A14,Table1[ID],0)),\"\")","v":""},"",{"$f":"_xlfn.IFNA(INDEX(Table1[HP/LP],MATCH($A14,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[IS],MATCH($A14,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[Note],MATCH($A14,Table1[ID],0)),\"\")","v":""},{"$f":"_xlfn.IFNA(INDEX(Table1[TM],MATCH($A14,Table1[ID],0)),\"\")","v":""},null,""]
[""]

{"sheet":"Vault","index":2,"n_rows":30,"n_cols":15,"rows_kept":30,"cut":false,"hidden":false,"merged":[[26,1,26,2],[27,1,27,2]]}
["Loc","Target","Pail","Assay 1\n[mSv/h]","A1 date","Assay 2\n[mSv/h]","A2 date","Assay 3\n[mSv/h]","A3 date","Assay 4\n[mSv/h]","A4 date","Assay 5\n[mSv/h]","A5 date","Assayed","Comment"]
["1A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A2,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A2,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A2,Table1[Vault location],0))))","v":"UC#38"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B2,Table1[Target ID],0)))","v":274},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B2,Table1[Target ID],0))/1000, \"\"))","v":33.299999999999997},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B2,Table1[Target ID],0)), \"\"))","v":"2022-09-15"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B2,Table1[Target ID],0))/1000, \"\"))","v":4.78},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B2,Table1[Target ID],0)), \"\"))","v":"2022-12-16"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B2,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B2,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B2,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B2,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B2,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B2,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B2,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B2,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["1B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A3,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A3,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A3,Table1[Vault location],0))))","v":"UC#40"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B3,Table1[Target ID],0)))","v":278},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B3,Table1[Target ID],0))/1000, \"\"))","v":15.6},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B3,Table1[Target ID],0)), \"\"))","v":"2023-01-11"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B3,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B3,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B3,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B3,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B3,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B3,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B3,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B3,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B3,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B3,Table1[Target ID],0)))","v":"contains one proton beam window without copper cooling lines in addition to the target\n\nThis pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["1C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A4,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A4,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A4,Table1[Vault location],0))))","v":"UC#41"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B4,Table1[Target ID],0)))","v":231},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B4,Table1[Target ID],0))/1000, \"\"))","v":14},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B4,Table1[Target ID],0)), \"\"))","v":"2023-01-30"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B4,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B4,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B4,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B4,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B4,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B4,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B4,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B4,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B4,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B4,Table1[Target ID],0)))","v":"Pail is likely contaminated, Contains two proton beam window without copper cooling lines in addition to the target\n\nThis pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["2A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A5,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A5,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A5,Table1[Vault location],0))))","v":"UC#36"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B5,Table1[Target ID],0)))","v":265},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B5,Table1[Target ID],0))/1000, \"\"))","v":19.600000000000001},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B5,Table1[Target ID],0)), \"\"))","v":"2022-01-12"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B5,Table1[Target ID],0))/1000, \"\"))","v":10.7},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B5,Table1[Target ID],0)), \"\"))","v":"2022-01-28"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B5,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B5,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B5,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B5,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B5,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B5,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B5,Table1[Target ID],0)))","v":"Measured"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B5,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["2B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A6,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A6,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A6,Table1[Vault location],0))))","v":"SiC#42"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B6,Table1[Target ID],0)))","v":271},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B6,Table1[Target ID],0))/1000, \"\"))","v":9.14},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B6,Table1[Target ID],0)), \"\"))","v":"2022-07-06"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B6,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B6,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B6,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B6,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B6,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B6,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B6,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B6,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B6,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B6,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["2C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A7,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A7,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A7,Table1[Vault location],0))))","v":"C#3"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B7,Table1[Target ID],0)))","v":270},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B7,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B7,Table1[Target ID],0))/1000, \"\"))","v":37.9},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B7,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B7,Table1[Target ID],0)), \"\"))","v":"2021-11-10"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B7,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B7,Table1[Target ID],0))/1000, \"\"))","v":10.8},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B7,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B7,Table1[Target ID],0)), \"\"))","v":"2022-01-28"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B7,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B7,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B7,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B7,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B7,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B7,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B7,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B7,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B7,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B7,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B7,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B7,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B7,Table1[Target ID],0)))","v":"Measured"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B7,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["3A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A8,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A8,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A8,Table1[Vault location],0))))","v":"TiC#5"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B8,Table1[Target ID],0)))","v":279},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B8,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B8,Table1[Target ID],0))/1000, \"\"))","v":40},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B8,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B8,Table1[Target ID],0)), \"\"))","v":"2023-06-21"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B8,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B8,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B8,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B8,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B8,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B8,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B8,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B8,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B8,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B8,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B8,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B8,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B8,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B8,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B8,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B8,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B8,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B8,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["3B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A9,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A9,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A9,Table1[Vault location],0))))","v":"Ta#63"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B9,Table1[Target ID],0)))","v":266},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B9,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B9,Table1[Target ID],0))/1000, \"\"))","v":410},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B9,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B9,Table1[Target ID],0)), \"\"))","v":"20/01/2022"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B9,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B9,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B9,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B9,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B9,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B9,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B9,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B9,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B9,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B9,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B9,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B9,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B9,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B9,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B9,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B9,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B9,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B9,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["3C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A10,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A10,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A10,Table1[Vault location],0))))","v":"SiC#45"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B10,Table1[Target ID],0)))","v":280},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B10,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B10,Table1[Target ID],0))/1000, \"\"))","v":138},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B10,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B10,Table1[Target ID],0)), \"\"))","v":"2023-07-27"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B10,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B10,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B10,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B10,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B10,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B10,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B10,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B10,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B10,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B10,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B10,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B10,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B10,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B10,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B10,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B10,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B10,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B10,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["4A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A11,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A11,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A11,Table1[Vault location],0))))","v":"SiC#44"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B11,Table1[Target ID],0)))","v":275},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B11,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B11,Table1[Target ID],0))/1000, \"\"))","v":42.6},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B11,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B11,Table1[Target ID],0)), \"\"))","v":"2022-10-13"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B11,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B11,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B11,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B11,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B11,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B11,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B11,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B11,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B11,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B11,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B11,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B11,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B11,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B11,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B11,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B11,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B11,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B11,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["4B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A12,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A12,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A12,Table1[Vault location],0))))","v":"UC#39"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B12,Table1[Target ID],0)))","v":276},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B12,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B12,Table1[Target ID],0))/1000, \"\"))","v":14.4},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B12,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B12,Table1[Target ID],0)), \"\"))","v":"2022-11-03"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B12,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B12,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B12,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B12,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B12,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B12,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B12,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B12,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B12,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B12,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B12,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B12,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B12,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B12,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B12,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B12,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B12,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B12,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["4C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A13,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A13,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A13,Table1[Vault location],0))))","v":"C#4"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B13,Table1[Target ID],0)))","v":277},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B13,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B13,Table1[Target ID],0))/1000, \"\"))","v":164},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B13,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B13,Table1[Target ID],0)), \"\"))","v":"2022-11-24"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B13,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B13,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B13,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B13,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B13,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B13,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B13,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B13,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B13,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B13,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B13,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B13,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B13,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B13,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B13,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B13,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B13,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B13,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["5A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A14,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A14,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A14,Table1[Vault location],0))))","v":"SiC#43"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B14,Table1[Target ID],0)))","v":272},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B14,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B14,Table1[Target ID],0))/1000, \"\"))","v":47.8},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B14,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B14,Table1[Target ID],0)), \"\"))","v":"28/07/2022"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B14,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B14,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B14,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B14,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B14,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B14,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B14,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B14,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B14,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B14,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B14,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B14,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B14,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B14,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B14,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B14,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B14,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B14,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["5B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A15,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A15,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A15,Table1[Vault location],0))))","v":"SiC#41"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B15,Table1[Target ID],0)))","v":260},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B15,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B15,Table1[Target ID],0))/1000, \"\"))","v":33.1},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B15,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B15,Table1[Target ID],0)), \"\"))","v":"13/10/2021"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B15,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B15,Table1[Target ID],0))/1000, \"\"))","v":7.8},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B15,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B15,Table1[Target ID],0)), \"\"))","v":"2022-01-30"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B15,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B15,Table1[Target ID],0))/1000, \"\"))","v":1.46},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B15,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B15,Table1[Target ID],0)), \"\"))","v":"2022-12-16"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B15,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B15,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B15,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B15,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B15,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B15,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B15,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B15,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B15,Table1[Target ID],0)))","v":"Measured"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B15,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["5C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A16,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A16,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A16,Table1[Vault location],0))))","v":"Ta#64"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B16,Table1[Target ID],0)))","v":273},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B16,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B16,Table1[Target ID],0))/1000, \"\"))","v":86.6},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B16,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B16,Table1[Target ID],0)), \"\"))","v":"2022-08-18"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B16,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B16,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B16,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B16,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B16,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B16,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B16,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B16,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B16,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B16,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B16,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B16,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B16,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B16,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B16,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B16,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B16,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B16,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["6A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A17,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A17,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A17,Table1[Vault location],0))))","v":"TiC#6"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B17,Table1[Target ID],0)))","v":232},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B17,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B17,Table1[Target ID],0))/1000, \"\"))","v":151},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B17,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B17,Table1[Target ID],0)), \"\"))","v":"2023-08-23"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B17,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B17,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B17,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B17,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B17,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B17,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B17,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B17,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B17,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B17,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B17,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B17,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B17,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B17,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B17,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B17,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B17,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B17,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["6B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A18,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A18,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A18,Table1[Vault location],0))))","v":"UC#42"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B18,Table1[Target ID],0)))","v":282},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B18,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B18,Table1[Target ID],0))/1000, \"\"))","v":34.9},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B18,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B18,Table1[Target ID],0)), \"\"))","v":"2023-09-01"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B18,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B18,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B18,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B18,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B18,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B18,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B18,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B18,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B18,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B18,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B18,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B18,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B18,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B18,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B18,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B18,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B18,Table1[Target ID],0)))","v":0},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B18,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["6C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A19,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A19,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A19,Table1[Vault location],0))))","v":"Nb#9"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B19,Table1[Target ID],0)))","v":246},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B19,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B19,Table1[Target ID],0))/1000, \"\"))","v":149},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B19,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B19,Table1[Target ID],0)), \"\"))","v":"2021-01-21"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B19,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B19,Table1[Target ID],0))/1000, \"\"))","v":9.08},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B19,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B19,Table1[Target ID],0)), \"\"))","v":"2022-01-31"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B19,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B19,Table1[Target ID],0))/1000, \"\"))","v":1.98},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B19,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B19,Table1[Target ID],0)), \"\"))","v":"2022-12-16"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B19,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B19,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B19,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B19,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B19,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B19,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B19,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B19,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B19,Table1[Target ID],0)))","v":"Measured"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B19,Table1[Target ID],0)))","v":"This pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["7A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A20,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A20,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A20,Table1[Vault location],0))))","v":"Ta#62"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B20,Table1[Target ID],0)))","v":256},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B20,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B20,Table1[Target ID],0))/1000, \"\"))","v":58},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B20,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B20,Table1[Target ID],0)), \"\"))","v":"2021-09-17"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B20,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B20,Table1[Target ID],0))/1000, \"\"))","v":16.899999999999999},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B20,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B20,Table1[Target ID],0)), \"\"))","v":"2022-01-27"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B20,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B20,Table1[Target ID],0))/1000, \"\"))","v":3.6},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B20,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B20,Table1[Target ID],0)), \"\"))","v":" 2022-12-16"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B20,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B20,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B20,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B20,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B20,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B20,Table1[Target ID],0))/1000, \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B20,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B20,Table1[Target ID],0)), \"\"))","v":""},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B20,Table1[Target ID],0)))","v":"Measured"},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B20,Table1[Target ID],0)))","v":"2022-12-16 moved from 7A to 7B in vault. - AN Pail placed back in 7A. -TC\nDisc in bottom of pail was not installed pail will need repacking. This pail is likely contaminated and also contains 2A2M19.\n\nThis pail is of previous revision, not certified as lifting device. Prior to shipping, a 3\" loop must be crimped at the end of the wire rope."}]
["7B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A21,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A21,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A21,Table1[Vault location],0))))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B21,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B21,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B21,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B21,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B21,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B21,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B21,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B21,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B21,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B21,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B21,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B21,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B21,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B21,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B21,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B21,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B21,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B21,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B21,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B21,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B21,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B21,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B21,Table1[Target ID],0)))","v":" "}]
["7C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A22,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A22,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A22,Table1[Vault location],0))))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B22,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B22,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B22,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B22,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B22,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B22,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B22,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B22,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B22,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B22,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B22,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B22,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B22,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B22,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B22,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B22,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B22,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B22,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B22,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B22,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B22,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B22,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B22,Table1[Target ID],0)))","v":" "}]
["8A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A23,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A23,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A23,Table1[Vault location],0))))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B23,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B23,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B23,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B23,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B23,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B23,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B23,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B23,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B23,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B23,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B23,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B23,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B23,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B23,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B23,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B23,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B23,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B23,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B23,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B23,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B23,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B23,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B23,Table1[Target ID],0)))","v":" "}]
["8B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A24,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A24,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A24,Table1[Vault location],0))))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B24,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B24,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B24,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B24,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B24,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B24,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B24,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B24,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B24,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B24,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B24,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B24,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B24,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B24,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B24,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B24,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B24,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B24,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B24,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B24,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B24,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B24,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B24,Table1[Target ID],0)))","v":" "}]
["8C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A25,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A25,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A25,Table1[Vault location],0))))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B25,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B25,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B25,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B25,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B25,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B25,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B25,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B25,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B25,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B25,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B25,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B25,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B25,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B25,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B25,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B25,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B25,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B25,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B25,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B25,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B25,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B25,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table4[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B25,Table1[Target ID],0)))","v":" "}]
[]
[9,"TM4 optics tray 2018. TM2 source tray 2019",null,1.87,"2018-06-14",14,"2019-03-01",7.1,"2020-11-02",null,null,null,null,null,"In Source Tray Box. The 1.9 mSv/Hr value is just for the optics tray. All other values are for both Optics and Source tray."]
[10,"TM4 Source tray",null,22.1,"2019-06-10",null,null,null,null,null,null,null,null,null,"7.5 to 22.1 mSv/hr on 360 rotation."]
[]
[null,null,null,"Need to change pail to new design"]

{"sheet":"miniVault","index":3,"n_rows":6,"n_cols":15,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["Loc","Target","Pail","Assay 1\n[mSv/h]","A1 date","Assay 2\n[mSv/h]","A2 date","Assay 3\n[mSv/h]","A3 date","Assay 4\n[mSv/h]","A4 date","Assay 5\n[mSv/h]","A45date","Assayed","Comment"]
["M1",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A2,Table1[Mini Storage location],0))),\" \",IF(INDEX(Table1[Date removed from Mini Storage],MATCH(A2,Table1[Mini Storage location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A2,Table1[Mini Storage location],0))))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B2,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B2,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B2,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B2,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B2,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B2,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B2,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B2,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B2,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B2,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B2,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B2,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B2,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B2,Table1[Target ID],0)))","v":" "}]
["M2",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A3,Table1[Mini Storage location],0))),\" \",IF(INDEX(Table1[Date removed from Mini Storage],MATCH(A3,Table1[Mini Storage location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A3,Table1[Mini Storage location],0))))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B3,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B3,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B3,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B3,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B3,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B3,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B3,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B3,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B3,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B3,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B3,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B3,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B3,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B3,Table1[Target ID],0)))","v":" "}]
["M3",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A4,Table1[Mini Storage location],0))),\" \",IF(INDEX(Table1[Date removed from Mini Storage],MATCH(A4,Table1[Mini Storage location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A4,Table1[Mini Storage location],0))))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B4,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B4,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B4,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B4,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B4,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B4,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B4,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B4,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B4,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B4,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B4,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B4,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B4,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B4,Table1[Target ID],0)))","v":" "}]
["M4",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A5,Table1[Mini Storage location],0))),\" \",IF(INDEX(Table1[Date removed from Mini Storage],MATCH(A5,Table1[Mini Storage location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A5,Table1[Mini Storage location],0))))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B5,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B5,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B5,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B5,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B5,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B5,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B5,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B5,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B5,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B5,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B5,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B5,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B5,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B5,Table1[Target ID],0)))","v":" "}]
["M5",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A6,Table1[Mini Storage location],0))),\" \",IF(INDEX(Table1[Date removed from Mini Storage],MATCH(A6,Table1[Mini Storage location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A6,Table1[Mini Storage location],0))))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Pail],MATCH(B6,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 1\n'[uSv/h']@1m],MATCH(B6,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 1\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 1 Date],MATCH(B6,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 2\n'[uSv/h']@1m],MATCH(B6,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 2\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 2 Date],MATCH(B6,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 3\n'[uSv/h']@1m],MATCH(B6,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 3\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 3 Date],MATCH(B6,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 4\n'[uSv/h']@1m],MATCH(B6,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 4\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 4 Date],MATCH(B6,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 5\n'[uSv/h']@1m],MATCH(B6,Table1[Target ID],0))/1000, \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",IF(INDEX(Table1[Assay 5\n'[uSv/h']@1m]>0,MATCH(B6,Table1[Target ID],0)),INDEX(Table1[Assay 5 Date],MATCH(B6,Table1[Target ID],0)), \"\"))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Target Assayed],MATCH(B6,Table1[Target ID],0)))","v":" "},{"$f":"IF(Table47[[#This Row],[Target]]=\" \",\" \",INDEX(Table1[Vault comment],MATCH(B6,Table1[Target ID],0)))","v":" "}]

{"sheet":"Summary","index":4,"n_rows":141,"n_cols":6,"rows_kept":141,"cut":false,"hidden":false,"merged":[]}
["Target Module","Targets"]
["TM1",58]
["TM2",39]
["TM3",11]
["TM4",60]
["Total",168]
[]
["Materials","Targets"]
["Al2O3",1]
["CaO",2]
["CaZrO3",2]
["Nb",9]
["Nb5SiC3",1]
["NiO",2]
["nSiC",1]
["SiC",39]
["Ta",61]
["TaC",1]
["ThO",1]
["TiC",4]
["UC",31]
["UO2",3]
["ZrC",8]
["Total",166]
[]
["Year","Targets"]
[1998,2]
[1999,2]
[2000,3]
[2001,3]
[2002,4]
[2003,6]
[2004,8]
[2005,8]
[2006,9]
[2007,7]
[2008,7]
[2009,9]
[2010,11]
[2011,8]
[2012,9]
[2013,9]
[2014,10]
[2015,8]
[2016,11]
[2017,10]
[2018,9]
[2019,8]
[2020,7]
["Total",168]
[]
["Row Labels","Sum of Net Charge "]
[1998,400]
[1999,10029.799999999999]
[2000,7009.07]
[2001,37179.03]
[2002,76995.95]
[2003,83179.259999999995]
[2004,107526.55]
[2005,127578.86]
[2006,175878.20000000004]
[2007,174857.37]
[2008,162771.80000000002]
[2009,139771.51]
[2010,214835.62]
[2011,182686.79]
[2012,132813.83999999997]
[2013,136661.14000000001]
[2014,170920.74]
[2015,144489.68]
[2016,167122.07]
[2017,192167.19]
[2018,70859.48]
[2019,118652.73]
[2020]
["SUM",2634386.6799999997]
[]
["Count of Material","Column Labels"]
["Row Labels","TM1","TM2","TM3","TM4","Grand Total"]
[1998,2,null,null,null,2]
[1999,2,null,null,null,2]
[2000,3,null,null,null,3]
[2001,3,null,null,null,3]
[2002,4,null,null,null,4]
[2003,4,1,1,null,6]
[2004,5,2,1,null,8]
[2005,3,4,1,null,8]
[2006,5,3,null,1,9]
[2007,1,3,null,3,7]
[2008,3,1,null,3,7]
[2009,2,null,2,5,9]
[2010,3,null,3,5,11]
[2011,4,null,null,4,8]
[2012,5,null,null,4,9]
[2013,3,null,1,5,9]
[2014,4,null,2,4,10]
[2015,1,2,null,5,8]
[2016,1,5,null,5,11]
[2017,null,5,null,5,10]
[2018,null,4,null,5,9]
[2019,null,5,null,3,8]
[2020,null,4,null,3,7]
["Grand Total",58,39,11,60,168]
[]
["Count of Target ID","Column Labels"]
["Row Labels","UC","Grand Total"]
[2010,1,1]
[2011,2,2]
[2012,2,2]
[2013,3,3]
[2014,3,3]
[2015,3,3]
[2016,4,4]
[2017,3,3]
[2018,5,5]
[2019,3,3]
[2020,2,2]
["Grand Total",31,31]
[]
[]
[]
["TM","TM4"]
[]
[null,"Values"]
["Row Labels","Max of BIAS","Average of BIAS","Min of BIAS"]
[2006]
[2007]
[2008]
[2009]
[2010,36.6,30.15,28]
[2011,51,35.75,28]
[2012,53,39.475000000000001,28]
[2013,51,28.3,20]
[2014,30,27.625,24.5]
[2015,40,29.7,22.5]
[2016,42,29.2,20]
[2017,40,32.6,25]
[2018,40,28,22.5]
[2019,30,27.5,25]
[2020]
["Grand Total",53,30.837209302325583,20]

{"sheet":"VaultPlan","index":5,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":false,"merged":[]}
["Location","Target","Days remaining",".25Y",".5Y",".75Y","1Y","1.25Y","1.5Y","1.75Y","2Y"]
["1A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A2,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A2,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A2,Table1[Vault location],0))))","v":"UC#38"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B2,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B2,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B2,Table1[Target ID],0)),NA()))","v":241.90288000000146},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":150.90288000000146},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":59.90288000000146},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-31.09711999999854},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-123.09711999999854},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-214.09711999999854},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-305.09711999999854},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-396.09711999999854},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-488.09711999999854}]
["1B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A3,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A3,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A3,Table1[Vault location],0))))","v":"UC#40"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B3,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B3,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B3,Table1[Target ID],0)),NA()))","v":201.96515999999974},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":110.96515999999974},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":19.965159999999742},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-71.034840000000258},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-163.03484000000026},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-254.03484000000026},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-345.03484000000026},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-436.03484000000026},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-528.03484000000026}]
["1C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A4,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A4,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A4,Table1[Vault location],0))))","v":"UC#41"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B4,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B4,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B4,Table1[Target ID],0)),NA()))","v":52.936639999999898},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":-38.063360000000102},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":-129.0633600000001},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-220.0633600000001},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-312.0633600000001},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-403.0633600000001},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-494.0633600000001},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-585.0633600000001},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-677.0633600000001}]
["2A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A5,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A5,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A5,Table1[Vault location],0))))","v":"UC#36"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B5,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B5,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B5,Table1[Target ID],0)),NA()))","v":-194.46024000000034},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":-285.46024000000034},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":-376.46024000000034},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-467.46024000000034},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-559.46024000000034},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-650.46024000000034},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-741.46024000000034},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-832.46024000000034},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-924.46024000000034}]
["2B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A6,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A6,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A6,Table1[Vault location],0))))","v":"SiC#42"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B6,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B6,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B6,Table1[Target ID],0)),NA()))","v":-378.25392000000284},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":-469.25392000000284},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":-560.25392000000284},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-651.25392000000284},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-743.25392000000284},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-834.25392000000284},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-925.25392000000284},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-1016.2539200000028},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-1108.2539200000028}]
["2C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A7,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A7,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A7,Table1[Vault location],0))))","v":"C#3"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B7,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B7,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B7,Table1[Target ID],0)),NA()))","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":{"$error":"#N/A"}}]
["3A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A8,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A8,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A8,Table1[Vault location],0))))","v":"TiC#5"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B8,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B8,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B8,Table1[Target ID],0)),NA()))","v":159.97983999999997},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":68.979839999999967},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":-22.020160000000033},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-113.02016000000003},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-205.02016000000003},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-296.02016000000003},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-387.02016000000003},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-478.02016000000003},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-570.02016000000003}]
["3B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A9,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A9,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A9,Table1[Vault location],0))))","v":"Ta#63"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B9,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B9,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B9,Table1[Target ID],0)),NA()))","v":-230.02736000000004},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":-321.02736000000004},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":-412.02736000000004},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-503.02736000000004},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-595.02736000000004},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-686.02736000000004},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-777.02736000000004},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-868.02736000000004},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-960.02736000000004}]
["3C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A10,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A10,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A10,Table1[Vault location],0))))","v":"SiC#45"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B10,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B10,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B10,Table1[Target ID],0)),NA()))","v":1356.4164799999999},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":1265.4164799999999},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":1174.4164799999999},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":1083.4164799999999},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":991.41647999999986},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":900.41647999999986},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":809.41647999999986},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":718.41647999999986},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":626.41647999999986}]
["4A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A11,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A11,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A11,Table1[Vault location],0))))","v":"SiC#44"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B11,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B11,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B11,Table1[Target ID],0)),NA()))","v":193.1359999999986},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":102.1359999999986},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":11.135999999998603},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-79.864000000001397},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-171.8640000000014},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-262.8640000000014},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-353.8640000000014},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-444.8640000000014},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-536.8640000000014}]
["4B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A12,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A12,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A12,Table1[Vault location],0))))","v":"UC#39"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B12,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B12,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B12,Table1[Target ID],0)),NA()))","v":-17.463960000000952},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":-108.46396000000095},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":-199.46396000000095},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-290.46396000000095},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-382.46396000000095},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-473.46396000000095},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-564.46396000000095},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-655.46396000000095},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-747.46396000000095}]
["4C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A13,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A13,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A13,Table1[Vault location],0))))","v":"C#4"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B13,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B13,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B13,Table1[Target ID],0)),NA()))","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":{"$error":"#N/A"}}]
["5A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A14,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A14,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A14,Table1[Vault location],0))))","v":"SiC#43"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B14,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B14,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B14,Table1[Target ID],0)),NA()))","v":{"$error":"#VALUE!"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":{"$error":"#VALUE!"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":{"$error":"#VALUE!"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":{"$error":"#VALUE!"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":{"$error":"#VALUE!"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":{"$error":"#VALUE!"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":{"$error":"#VALUE!"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":{"$error":"#VALUE!"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":{"$error":"#VALUE!"}}]
["5B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A15,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A15,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A15,Table1[Vault location],0))))","v":"SiC#41"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B15,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B15,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B15,Table1[Target ID],0)),NA()))","v":-415.78399999999965},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":-506.78399999999965},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":-597.78399999999965},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-688.78399999999965},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-780.78399999999965},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-871.78399999999965},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-962.78399999999965},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-1053.7839999999997},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-1145.7839999999997}]
["5C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A16,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A16,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A16,Table1[Vault location],0))))","v":"Ta#64"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B16,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B16,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B16,Table1[Target ID],0)),NA()))","v":26.982120000000577},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":-64.017879999999423},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":-155.01787999999942},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-246.01787999999942},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-338.01787999999942},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-429.01787999999942},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-520.01787999999942},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-611.01787999999942},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-703.01787999999942}]
["6A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A17,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A17,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A17,Table1[Vault location],0))))","v":"TiC#6"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B17,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B17,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B17,Table1[Target ID],0)),NA()))","v":681.39199999999983},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":590.39199999999983},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":499.39199999999983},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":408.39199999999983},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":316.39199999999983},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":225.39199999999983},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":134.39199999999983},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":43.391999999999825},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-48.608000000000175}]
["6B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A18,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A18,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A18,Table1[Vault location],0))))","v":"UC#42"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B18,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B18,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B18,Table1[Target ID],0)),NA()))","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":{"$error":"#N/A"}},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":{"$error":"#N/A"}}]
["6C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A19,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A19,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A19,Table1[Vault location],0))))","v":"Nb#9"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B19,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B19,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B19,Table1[Target ID],0)),NA()))","v":-555.76299999999901},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":-646.76299999999901},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":-737.76299999999901},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-828.76299999999901},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-920.76299999999901},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-1011.762999999999},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-1102.762999999999},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-1193.762999999999},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-1285.762999999999}]
["7A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A20,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A20,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A20,Table1[Vault location],0))))","v":"Ta#62"},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B20,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B20,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B20,Table1[Target ID],0)),NA()))","v":-290.86155999999755},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":-381.86155999999755},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":-472.86155999999755},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":-563.86155999999755},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":-655.86155999999755},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":-746.86155999999755},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":-837.86155999999755},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":-928.86155999999755},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":-1020.8615599999976}]
["7B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A21,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A21,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A21,Table1[Vault location],0))))","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B21,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B21,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B21,Table1[Target ID],0)),NA()))","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":" "}]
["7C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A22,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A22,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A22,Table1[Vault location],0))))","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B22,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B22,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B22,Table1[Target ID],0)),NA()))","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":" "}]
["8A",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A23,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A23,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A23,Table1[Vault location],0))))","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B23,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B23,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B23,Table1[Target ID],0)),NA()))","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":" "}]
["8B",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A24,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A24,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A24,Table1[Vault location],0))))","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B24,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B24,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B24,Table1[Target ID],0)),NA()))","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":" "}]
["8C",{"$f":"IF(ISNA(INDEX(Table1[Target ID],MATCH(A25,Table1[Vault location],0))),\" \",IF(INDEX(Table1[Date of being sent to Mini Storage],MATCH(A25,Table1[Vault location],0))>0, \" \",INDEX(Table1[Target ID],MATCH(A25,Table1[Vault location],0))))","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",IF(INDEX(Table1[Offline p+],MATCH(VaultPlan!B25,Table1[Target ID],0)),INDEX(Table1[Optimistic],MATCH(VaultPlan!B25,Table1[Target ID],0))-TODAY()+INDEX(Table1[Offline p+],MATCH(VaultPlan!B25,Table1[Target ID],0)),NA()))","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[Days remaining]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.25Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.5Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[.75Y]]-92)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.25Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.5Y]]-91)","v":" "},{"$f":"IF(Table2[[#This Row],[Target]]=\" \", \" \",Table2[[#This Row],[1.75Y]]-92)","v":" "}]
[]
["Other"]
["Remaining",null,{"$f":"COUNTIF(Table2[Days remaining],\">0\")+C27","v":8},{"$f":"COUNTIF(Table2[.25Y],\">0\")+D27","v":6},{"$f":"COUNTIF(Table2[.5Y],\">0\")+E27","v":5},{"$f":"COUNTIF(Table2[.75Y],\">0\")+F27","v":2},{"$f":"COUNTIF(Table2[1Y],\">0\")+G27","v":2},{"$f":"COUNTIF(Table2[1.25Y],\">0\")+H27","v":2},{"$f":"COUNTIF(Table2[1.5Y],\">0\")+I27","v":2},{"$f":"COUNTIF(Table2[1.75Y],\">0\")+J27","v":2},{"$f":"COUNTIF(Table2[2Y],\">0\")+K27","v":1}]
[]
[null,"Target","Days to decay",".25Y",".5Y",".75Y","1Y","1.25Y","1.5Y","1.75Y","2Y"]
[null,"UC#32",{"$f":"INDEX(Table1[Estimated ship days],MATCH(VaultPlan!B31,Table1[Target ID],0))","v":474.24},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-91+C31,\" \")","v":-410.76},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-91*2+C31,\" \")","v":-501.76},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-91*3+C31,\" \")","v":-592.76},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-365<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-365+C31,NA())","v":-684.76},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-365-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-365-91+C31,NA())","v":-775.76},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-365-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-365-91*2+C31,NA())","v":-866.76},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-365-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-365-91*3+C31,NA())","v":-957.76},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-365*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B31,Table1[Target ID],0))-TODAY()-365*2+C31,NA())","v":-1049.76}]
[null,"UC#33",{"$f":"INDEX(Table1[Estimated ship days],MATCH(VaultPlan!B32,Table1[Target ID],0))","v":1057.92},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-91+C32,\" \")","v":201.92000000000007},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-91*2+C32,\" \")","v":110.92000000000007},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-91*3+C32,\" \")","v":19.920000000000073},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-365<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-365+C32,NA())","v":-72.079999999999927},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-365-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-365-91+C32,NA())","v":-163.07999999999993},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-365-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-365-91*2+C32,NA())","v":-254.07999999999993},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-365-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-365-91*3+C32,NA())","v":-345.07999999999993},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-365*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B32,Table1[Target ID],0))-TODAY()-365*2+C32,NA())","v":-437.07999999999993}]
[null,"Ta#62",{"$f":"INDEX(Table1[Estimated ship days],MATCH(VaultPlan!B33,Table1[Target ID],0))","v":752.64},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-91+C33,\" \")","v":-75.360000000000014},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-91*2+C33,\" \")","v":-166.36},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-91*3+C33,\" \")","v":-257.36},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-365<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-365+C33,NA())","v":-349.36},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-365-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-365-91+C33,NA())","v":-440.36},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-365-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-365-91*2+C33,NA())","v":-531.36},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-365-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-365-91*3+C33,NA())","v":-622.36},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-365*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B33,Table1[Target ID],0))-TODAY()-365*2+C33,NA())","v":-714.36}]
[null,"UC#34",{"$f":"INDEX(Table1[Estimated ship days],MATCH(VaultPlan!B34,Table1[Target ID],0))","v":729.6},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-91+C34,\" \")","v":-78.399999999999977},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-91*2+C34,\" \")","v":-169.39999999999998},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-91*3+C34,\" \")","v":-260.39999999999998},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-365<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-365+C34,NA())","v":-352.4},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-365-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-365-91+C34,NA())","v":-443.4},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-365-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-365-91*2+C34,NA())","v":-534.4},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-365-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-365-91*3+C34,NA())","v":-625.4},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-365*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B34,Table1[Target ID],0))-TODAY()-365*2+C34,NA())","v":-717.4}]
[null,"SIC#40",{"$f":"INDEX(Table1[Estimated ship days],MATCH(VaultPlan!B35,Table1[Target ID],0))","v":1313.28},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-91+C35,\" \")","v":517.28},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-91*2+C35,\" \")","v":426.28},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-91*3+C35,\" \")","v":335.28},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-365<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-365+C35,NA())","v":243.27999999999997},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-365-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-365-91+C35,NA())","v":152.27999999999997},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-365-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-365-91*2+C35,NA())","v":61.279999999999973},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-365-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-365-91*3+C35,NA())","v":-29.720000000000027},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-365*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B35,Table1[Target ID],0))-TODAY()-365*2+C35,NA())","v":-121.72000000000003}]
[null,null,{"$f":"INDEX(Table1[Estimated ship days],MATCH(VaultPlan!B36,Table1[Target ID],0))","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-91+C36,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-91*2+C36,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-91*3+C36,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-365<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-365+C36,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-365-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-365-91+C36,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-365-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-365-91*2+C36,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-365-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-365-91*3+C36,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-365*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B36,Table1[Target ID],0))-TODAY()-365*2+C36,NA())","v":{"$error":"#N/A"}}]
[null,null,{"$f":"INDEX(Table1[Estimated ship days],MATCH(VaultPlan!B37,Table1[Target ID],0))","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-91+C37,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-91*2+C37,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-91*3+C37,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-365<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-365+C37,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-365-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-365-91+C37,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-365-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-365-91*2+C37,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-365-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-365-91*3+C37,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-365*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B37,Table1[Target ID],0))-TODAY()-365*2+C37,NA())","v":{"$error":"#N/A"}}]
[null,null,{"$f":"INDEX(Table1[Estimated ship days],MATCH(VaultPlan!B38,Table1[Target ID],0))","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-91+C38,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-91*2+C38,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-91*3+C38,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-365<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-365+C38,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-365-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-365-91+C38,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-365-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-365-91*2+C38,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-365-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-365-91*3+C38,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-365*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B38,Table1[Target ID],0))-TODAY()-365*2+C38,NA())","v":{"$error":"#N/A"}}]
[null,null,{"$f":"INDEX(Table1[Estimated ship days],MATCH(VaultPlan!B39,Table1[Target ID],0))","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-91+C39,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-91*2+C39,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-91*3+C39,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-365<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-365+C39,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-365-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-365-91+C39,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-365-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-365-91*2+C39,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-365-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-365-91*3+C39,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-365*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B39,Table1[Target ID],0))-TODAY()-365*2+C39,NA())","v":{"$error":"#N/A"}}]
[null,null,{"$f":"INDEX(Table1[Estimated ship days],MATCH(VaultPlan!B40,Table1[Target ID],0))","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-91+C40,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-91*2+C40,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-91*3+C40,\" \")","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-365<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-365+C40,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-365-91<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-365-91+C40,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-365-91*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-365-91*2+C40,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-365-91*3<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-365-91*3+C40,NA())","v":{"$error":"#N/A"}},{"$f":"IF(INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-365*2<0,INDEX(Table1[Schedule end],MATCH(VaultPlan!B40,Table1[Target ID],0))-TODAY()-365*2+C40,NA())","v":{"$error":"#N/A"}}]
[]
["Date",null,{"$f":"TODAY()","v":"2023-09-01"},{"$f":"C42+91","v":"2023-12-01"},{"$f":"D42+91","v":"2024-03-01"},{"$f":"E42+91","v":"2024-05-31"},"2024-08-30","2024-11-29","2025-02-28","2025-05-30","2025-08-29"]
["Remaining",null,{"$f":"C28","v":8},{"$f":"COUNTIF(D31:D40,\">0\")+D28","v":8},7,4,3,3,3,2,1]
["Shippable",null,{"$f":"COUNTIF(Table2[Days remaining],\"<0\")","v":7},{"$f":"COUNTIF(Table3[.25Y],\"<0\")+COUNTIF(Table2[.25Y],\"<0\")","v":12},{"$f":"COUNTIF(Table3[.5Y],\"<0\")+COUNTIF(Table2[.5Y],\"<0\")","v":13},{"$f":"COUNTIF(Table3[.75Y],\"<0\")+COUNTIF(Table2[.75Y],\"<0\")","v":16},{"$f":"COUNTIF(Table3[1Y],\"<0\")+COUNTIF(Table2[1Y],\"<0\")","v":17},{"$f":"COUNTIF(Table3[1.25Y],\"<0\")+COUNTIF(Table2[1.25Y],\"<0\")","v":17},{"$f":"COUNTIF(Table3[1.5Y],\"<0\")+COUNTIF(Table2[1.5Y],\"<0\")","v":17},{"$f":"COUNTIF(Table3[1.75Y],\"<0\")+COUNTIF(Table2[1.75Y],\"<0\")","v":18},{"$f":"COUNTIF(Table3[2Y],\"<0\")+COUNTIF(Table2[2Y],\"<0\")","v":19}]
["Remaining [y]",null,{"$f":"(SUMIF(C2:C25,\">0\"))/365","v":7.9855099178082192},{"$f":"(SUMIF(D2:D25,\">0\")+SUMIF(D31:D40,\">0\"))/365","v":8.2410749589041075},{"$f":"(SUMIF(E2:E25,\">0\")+SUMIF(E31:E40,\">0\"))/365","v":6.3068836164383546},5.0602972054794515,4.2495574794520543,3.5016122739726017,2.7536670684931499,2.0871465205479445,1.7162095342465751]

{"sheet":"Pails","index":6,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Number","Vendor","Pail prod #","Lid prod #","Lock ring prod #","UN Rating","TRIUMF PO"]
[200,"TheCaryCompany","26WMA6","26WA3L","Not Used","UN1A2/Y1.5/100",3045431]
[201,"TheCaryCompany","26WMA6","26WA3L","Not Used","UN1A2/Y1.5/100",3045431]
[202,"TheCaryCompany","26WMA6","26WA3L","Not Used","UN1A2/Y1.5/100",3045431]
[203,"TheCaryCompany","26WMA6","26WA3L","Not Used","UN1A2/Y1.5/100",3045431]
[204,"TheCaryCompany","26WMA6","26WA3L","Not Used","UN1A2/Y1.5/100",3045431]
[205,"TheCaryCompany","26WMA6","26WA3L","Not Used","UN1A2/Y1.5/100",3045431]
[206,"TheCaryCompany","26WMA6","26WA3L","Not Used","UN1A2/Y1.5/100",3045431]
[207,"TheCaryCompany","26WMA6","26WA3L","Not Used","UN1A2/Y1.5/100",3045431]
[208,"TheCaryCompany","26WMA6","26WA3L","Not Used","UN1A2/Y1.5/100",3045431]
[209,"TheCaryCompany","26WMA6","26WA3L","Not Used","UN1A2/Y1.5/100",3045431]
[]
[]
["Lids and Pails have the same numbers attached to them."]
["Numbers started from 200 2018-09-25 (new pails)"]